From 3c1dc22162d673d595855d24f95200ed2643f88f Mon Sep 17 00:00:00 2001
From: Frank Sae <Frank.Sae@motor-comm.com>
Date: Sat, 28 Jan 2023 14:35:58 +0800
Subject: [PATCH] net: phy: motorcomm: change the phy id of yt8521 and yt8531s
 to lowercase

The phy id is usually defined in lower case.

Signed-off-by: Frank Sae <Frank.Sae@motor-comm.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Link: https://lore.kernel.org/r/20230128063558.5850-2-Frank.Sae@motor-comm.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/phy/motorcomm.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/phy/motorcomm.c
+++ b/drivers/net/phy/motorcomm.c
@@ -12,8 +12,8 @@
 #include <linux/phy.h>
 
 #define PHY_ID_YT8511		0x0000010a
-#define PHY_ID_YT8521		0x0000011A
-#define PHY_ID_YT8531S		0x4F51E91A
+#define PHY_ID_YT8521		0x0000011a
+#define PHY_ID_YT8531S		0x4f51e91a
 
 /* YT8521/YT8531S Register Overview
  *	UTP Register space	|	FIBER Register space
