From 22ae3b2ee3293278e647877b269a5aebad3f077d Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Thu, 27 May 2021 11:46:30 +0100
Subject: [PATCH] Allow RESET_BRCMSTB on ARCH_BCM2835

---
 drivers/reset/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/reset/Kconfig
+++ b/drivers/reset/Kconfig
@@ -51,7 +51,7 @@ config RESET_BERLIN
 
 config RESET_BRCMSTB
 	tristate "Broadcom STB reset controller"
-	depends on ARCH_BRCMSTB || COMPILE_TEST
+	depends on ARCH_BRCMSTB || ARCH_BCM2835 || COMPILE_TEST
 	default ARCH_BRCMSTB
 	help
 	  This enables the reset controller driver for Broadcom STB SoCs using
