From e4d7544ce092807e8c5aeb618cec30e2eb9b40c2 Mon Sep 17 00:00:00 2001
From: Mantas Pucka <mantas@8devices.com>
Date: Mon, 24 Apr 2023 15:13:32 +0300
Subject: [PATCH 3/3] arm64: dts: qcom: ipq6018: add SDHCI node

IPQ6018 has one SD/eMMC controller, add node for it.

Signed-off-by: Mantas Pucka <mantas@8devices.com>
Tested-by: Robert Marko <robimarko@gmail.com>
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 23 +++++++++++++++++++++++
 1 file changed, 23 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -469,6 +469,29 @@
 			};
 		};
 
+		sdhc_1: mmc@7804000 {
+			compatible = "qcom,ipq6018-sdhci", "qcom,sdhci-msm-v5";
+			reg = <0x0 0x07804000 0x0 0x1000>,
+			      <0x0 0x07805000 0x0 0x1000>,
+			      <0x0 0x07808000 0x0 0x2000>;
+			reg-names = "hc", "cqhci", "ice";
+
+			interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "hc_irq", "pwr_irq";
+
+			clocks = <&gcc GCC_SDCC1_AHB_CLK>,
+				 <&gcc GCC_SDCC1_APPS_CLK>,
+				 <&xo>,
+				 <&gcc GCC_SDCC1_ICE_CORE_CLK>;
+			clock-names = "iface", "core", "xo", "ice";
+
+			resets = <&gcc GCC_SDCC1_BCR>;
+			supports-cqe;
+			bus-width = <8>;
+			status = "disabled";
+		};
+
 		blsp_dma: dma-controller@7884000 {
 			compatible = "qcom,bam-v1.7.0";
 			reg = <0x0 0x07884000 0x0 0x2b000>;
