From: Daniel Golle <daniel@makrotopia.org>
Date: Tue, 10 Oct 2023 21:06:43 +0200
Subject: [PATCH net-next 2/2] net: ethernet: mediatek: use QDMA instead of
 ADMAv2 on MT7981 and MT7986

ADMA is plagued by RX hangs which can't easily detected and happen upon
receival of a corrupted package.
Use QDMA just like on netsys v1 which is also still present and usable, and
doesn't suffer from that problem.

Co-developed-by: Lorenzo Bianconi <lorenzo@kernel.org>
Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 46 ++++++++++-----------
 1 file changed, 23 insertions(+), 23 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -110,16 +110,16 @@ static const struct mtk_reg_map mt7986_r
 	.tx_irq_mask		= 0x461c,
 	.tx_irq_status		= 0x4618,
 	.pdma = {
-		.rx_ptr		= 0x6100,
-		.rx_cnt_cfg	= 0x6104,
-		.pcrx_ptr	= 0x6108,
-		.glo_cfg	= 0x6204,
-		.rst_idx	= 0x6208,
-		.delay_irq	= 0x620c,
-		.irq_status	= 0x6220,
-		.irq_mask	= 0x6228,
-		.adma_rx_dbg0	= 0x6238,
-		.int_grp	= 0x6250,
+		.rx_ptr		= 0x4100,
+		.rx_cnt_cfg	= 0x4104,
+		.pcrx_ptr	= 0x4108,
+		.glo_cfg	= 0x4204,
+		.rst_idx	= 0x4208,
+		.delay_irq	= 0x420c,
+		.irq_status	= 0x4220,
+		.irq_mask	= 0x4228,
+		.adma_rx_dbg0	= 0x4238,
+		.int_grp	= 0x4250,
 	},
 	.qdma = {
 		.qtx_cfg	= 0x4400,
@@ -1232,7 +1232,7 @@ static bool mtk_rx_get_desc(struct mtk_e
 	rxd->rxd1 = READ_ONCE(dma_rxd->rxd1);
 	rxd->rxd3 = READ_ONCE(dma_rxd->rxd3);
 	rxd->rxd4 = READ_ONCE(dma_rxd->rxd4);
-	if (mtk_is_netsys_v2_or_greater(eth)) {
+	if (mtk_is_netsys_v3_or_greater(eth)) {
 		rxd->rxd5 = READ_ONCE(dma_rxd->rxd5);
 		rxd->rxd6 = READ_ONCE(dma_rxd->rxd6);
 	}
@@ -2184,7 +2184,7 @@ static int mtk_poll_rx(struct napi_struc
 			break;
 
 		/* find out which mac the packet come from. values start at 1 */
-		if (mtk_is_netsys_v2_or_greater(eth)) {
+		if (mtk_is_netsys_v3_or_greater(eth)) {
 			u32 val = RX_DMA_GET_SPORT_V2(trxd.rxd5);
 
 			switch (val) {
@@ -2296,7 +2296,7 @@ static int mtk_poll_rx(struct napi_struc
 		skb->dev = netdev;
 		bytes += skb->len;
 
-		if (mtk_is_netsys_v2_or_greater(eth)) {
+		if (mtk_is_netsys_v3_or_greater(eth)) {
 			reason = FIELD_GET(MTK_RXD5_PPE_CPU_REASON, trxd.rxd5);
 			hash = trxd.rxd5 & MTK_RXD5_FOE_ENTRY;
 			if (hash != MTK_RXD5_FOE_ENTRY)
@@ -2846,7 +2846,7 @@ static int mtk_rx_alloc(struct mtk_eth *
 
 		rxd->rxd3 = 0;
 		rxd->rxd4 = 0;
-		if (mtk_is_netsys_v2_or_greater(eth)) {
+		if (mtk_is_netsys_v3_or_greater(eth)) {
 			rxd->rxd5 = 0;
 			rxd->rxd6 = 0;
 			rxd->rxd7 = 0;
@@ -4053,7 +4053,7 @@ static int mtk_hw_init(struct mtk_eth *e
 	else
 		mtk_hw_reset(eth);
 
-	if (mtk_is_netsys_v2_or_greater(eth)) {
+	if (mtk_is_netsys_v3_or_greater(eth)) {
 		/* Set FE to PDMAv2 if necessary */
 		val = mtk_r32(eth, MTK_FE_GLO_MISC);
 		mtk_w32(eth,  val | BIT(4), MTK_FE_GLO_MISC);
@@ -5400,11 +5400,11 @@ static const struct mtk_soc_data mt7981_
 		.dma_len_offset = 8,
 	},
 	.rx = {
-		.desc_size = sizeof(struct mtk_rx_dma_v2),
-		.irq_done_mask = MTK_RX_DONE_INT_V2,
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
 		.dma_l4_valid = RX_DMA_L4_VALID_V2,
-		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
-		.dma_len_offset = 8,
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
 	},
 };
 
@@ -5426,11 +5426,11 @@ static const struct mtk_soc_data mt7986_
 		.dma_len_offset = 8,
 	},
 	.rx = {
-		.desc_size = sizeof(struct mtk_rx_dma_v2),
-		.irq_done_mask = MTK_RX_DONE_INT_V2,
+		.desc_size = sizeof(struct mtk_rx_dma),
+		.irq_done_mask = MTK_RX_DONE_INT,
 		.dma_l4_valid = RX_DMA_L4_VALID_V2,
-		.dma_max_len = MTK_TX_DMA_BUF_LEN_V2,
-		.dma_len_offset = 8,
+		.dma_max_len = MTK_TX_DMA_BUF_LEN,
+		.dma_len_offset = 16,
 	},
 };
 
