From 2cd6022800d6da7822e169f3e6f7f790c1431445 Mon Sep 17 00:00:00 2001
From: Matthias Brugger <mbrugger@suse.com>
Date: Mon, 14 Nov 2022 13:16:53 +0100
Subject: [PATCH 05/19] arm64: dts: mediatek: mt7986: Add SoC compatible

Missing SoC compatible in the board file causes dt bindings check.

Signed-off-by: Matthias Brugger <mbrugger@suse.com>
Link: https://lore.kernel.org/r/20221114121653.14739-1-matthias.bgg@kernel.org
Signed-off-by: Matthias Brugger <matthias.bgg@gmail.com>
---
 arch/arm64/boot/dts/mediatek/mt7986a-rfb.dts | 2 +-
 arch/arm64/boot/dts/mediatek/mt7986a.dtsi    | 1 +
 arch/arm64/boot/dts/mediatek/mt7986b-rfb.dts | 2 +-
 arch/arm64/boot/dts/mediatek/mt7986b.dtsi    | 3 +++
 4 files changed, 6 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/mediatek/mt7986a-rfb.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7986a-rfb.dts
@@ -9,7 +9,7 @@
 
 / {
 	model = "MediaTek MT7986a RFB";
-	compatible = "mediatek,mt7986a-rfb";
+	compatible = "mediatek,mt7986a-rfb", "mediatek,mt7986a";
 
 	aliases {
 		serial0 = &uart0;
--- a/arch/arm64/boot/dts/mediatek/mt7986a.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7986a.dtsi
@@ -10,6 +10,7 @@
 #include <dt-bindings/reset/mt7986-resets.h>
 
 / {
+	compatible = "mediatek,mt7986a";
 	interrupt-parent = <&gic>;
 	#address-cells = <2>;
 	#size-cells = <2>;
--- a/arch/arm64/boot/dts/mediatek/mt7986b-rfb.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7986b-rfb.dts
@@ -9,7 +9,7 @@
 
 / {
 	model = "MediaTek MT7986b RFB";
-	compatible = "mediatek,mt7986b-rfb";
+	compatible = "mediatek,mt7986b-rfb", "mediatek,mt7986b";
 
 	aliases {
 		serial0 = &uart0;
--- a/arch/arm64/boot/dts/mediatek/mt7986b.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7986b.dtsi
@@ -5,6 +5,9 @@
  */
 
 #include "mt7986a.dtsi"
+/ {
+	compatible = "mediatek,mt7986b";
+};
 
 &pio {
 	compatible = "mediatek,mt7986b-pinctrl";
