From db5f028309ede13767e2ba356c1975ac37a4fd6c Mon Sep 17 00:00:00 2001
From: Andre Przywara <andre.przywara@arm.com>
Date: Mon, 31 Oct 2022 11:13:57 +0000
Subject: [PATCH] arm64: dts: allwinner: h616: OrangePi Zero 2: Add USB nodes

The OrangePi Zero 2 has one USB-A host port, VBUS is provided by
a GPIO controlled regulator.
The USB-C port is meant to power the board, but is also connected to
the USB 0 port, which we configure as an MUSB peripheral.

Signed-off-by: Andre Przywara <andre.przywara@arm.com>
Reviewed-by: Jernej Skrabec <jernej.skrabec@gmail.com>
Link: https://lore.kernel.org/r/20221031111358.3387297-7-andre.przywara@arm.com
Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 .../allwinner/sun50i-h616-orangepi-zero2.dts  | 41 +++++++++++++++++++
 1 file changed, 41 insertions(+)

--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2.dts
@@ -49,8 +49,24 @@
 		regulator-max-microvolt = <5000000>;
 		regulator-always-on;
 	};
+
+	reg_usb1_vbus: regulator-usb1-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&reg_vcc5v>;
+		enable-active-high;
+		gpio = <&pio 2 16 GPIO_ACTIVE_HIGH>; /* PC16 */
+	};
+};
+
+&ehci1 {
+	status = "okay";
 };
 
+/* USB 2 & 3 are on headers only. */
+
 &emac0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ext_rgmii_pins>;
@@ -76,6 +92,10 @@
 	status = "okay";
 };
 
+&ohci1 {
+	status = "okay";
+};
+
 &r_rsb {
 	status = "okay";
 
@@ -211,3 +231,24 @@
 	pinctrl-0 = <&uart0_ph_pins>;
 	status = "okay";
 };
+
+&usbotg {
+	/*
+	 * PHY0 pins are connected to a USB-C socket, but a role switch
+	 * is not implemented: both CC pins are pulled to GND.
+	 * The VBUS pins power the device, so a fixed peripheral mode
+	 * is the best choice.
+	 * The board can be powered via GPIOs, in this case port0 *can*
+	 * act as a host (with a cable/adapter ignoring CC), as VBUS is
+	 * then provided by the GPIOs. Any user of this setup would
+	 * need to adjust the DT accordingly: dr_mode set to "host",
+	 * enabling OHCI0 and EHCI0.
+	 */
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	usb1_vbus-supply = <&reg_usb1_vbus>;
+	status = "okay";
+};
