From 713a7ef9d73fca0f7fed122cb854d930b7a6ba5a Mon Sep 17 00:00:00 2001
From: Naushir Patuck <naush@raspberrypi.com>
Date: Wed, 21 Jun 2023 08:45:02 +0100
Subject: [PATCH] driver: media: i2c: imx477: Re-enable temperature sensor

The temperature sensor enable register write got lost at some point.
Re-enable it.

Signed-off-by: Naushir Patuck <naush@raspberrypi.com>
---
 drivers/media/i2c/imx477.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/media/i2c/imx477.c
+++ b/drivers/media/i2c/imx477.c
@@ -167,6 +167,7 @@ struct imx477_mode {
 static const struct imx477_reg mode_common_regs[] = {
 	{0x0136, 0x18},
 	{0x0137, 0x00},
+	{0x0138, 0x01},
 	{0xe000, 0x00},
 	{0xe07a, 0x01},
 	{0x0808, 0x02},
