// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/*
 * The hardware of this board family is most likely shared with other devices
 * from other manufacturers. Edimax appear to be the actual OEM.
 *
 * Sophos use the same exact board for the AP55C/AP100C, and AP55/AP100.
 * Yes, this means your AP55C is a 3x3 AP with a software lock, and your
 * AP55 is an AP100 with one missing antenna pigtail.
 *
 * AP55 and AP55C boards have different physical layouts, but are logically
 * almost identical. AP55/100 have an empty micro-USB OTG port footprint,
 * which may be possible to retrofit with some work.
 */

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_red;
		led-running = &led_status_green;
		led-upgrade = &led_status_red;
		label-mac-device = &eth0;
	};

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status_green: status_green {
			label = "green:status";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led_status_red: status_red {
			label = "red:status";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};

	reg_usb_vbus: reg_usb_vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio 11 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-boot-on;
		status = "disabled";
	};
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			art: partition@50000 {
				label = "art";
				reg = <0x050000 0x010000>;
				read-only;
			};

			config: partition@60000 {
				label = "config";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x070000 0xf90000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		reg = <4>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0xa6000000 0xa0000101 0xa0001313>;

	nvmem-cells = <&macaddr_config_201a>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii-id";
	phy-handle = <&phy4>;

	gmac_config: gmac-config {
		device = <&gmac>;

		rgmii-enabled = <1>;

		rxdv-delay = <3>;
		rxd-delay = <3>;
		txen-delay = <3>;
		txd-delay = <3>;
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&config {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_config_201a: macaddr@201a {
		reg = <0x201a 0x6>;
	};
};

&usb0 {
	vbus-supply = <&reg_usb_vbus>;
};
