#include "qcom-ipq8064-v2.0.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Netgear Nighthawk X4 R7500v2";
	compatible = "netgear,r7500v2", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	reserved-memory {
		rsvd@5fe00000 {
			reg = <0x5fe00000 0x200000>;
			reusable;
		};
	};

	aliases {
		mdio-gpio0 = &mdio0;

		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;
	};

	chosen {
		bootargs = "rootfstype=squashfs noinitrd";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wifi {
			label = "wifi";
			gpios = <&qcom_pinmux 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		usb1 {
			label = "amber:usb1";
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		usb3 {
			label = "amber:usb3";
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		status {
			label = "amber:status";
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		internet {
			label = "white:internet";
			gpios = <&qcom_pinmux 22 GPIO_ACTIVE_HIGH>;
		};

		wan {
			label = "white:wan";
			gpios = <&qcom_pinmux 23 GPIO_ACTIVE_HIGH>;
		};

		wps {
			label = "white:wps";
			gpios = <&qcom_pinmux 24 GPIO_ACTIVE_HIGH>;
		};

		esata {
			label = "white:esata";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
		};

		power: power {
			label = "white:power";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		wifi {
			label = "white:wifi";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_HIGH>;
		};
	};
};

&adm_dma {
	status = "okay";
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio6", "gpio54", "gpio65";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio7", "gpio8", "gpio9", "gpio22", "gpio23",
				"gpio24","gpio26", "gpio53", "gpio64";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	usb0_pwr_en_pins: usb0_pwr_en_pins {
		mux {
			pins = "gpio15";
			function = "gpio";
			drive-strength = <12>;
			bias-pull-down;
			output-high;
		};
	};

	usb1_pwr_en_pins: usb1_pwr_en_pins {
		mux {
			pins = "gpio16", "gpio68";
			function = "gpio";
			drive-strength = <12>;
			bias-pull-down;
			output-high;
		};
	};
};

&sata_phy {
	status = "okay";
};

&sata {
	status = "okay";
};

&usb3_0 {
	status = "okay";

	pinctrl-0 = <&usb0_pwr_en_pins>;
	pinctrl-names = "default";
};

&usb3_1 {
	status = "okay";

	pinctrl-0 = <&usb1_pwr_en_pins>;
	pinctrl-names = "default";
};

&pcie0 {
	status = "okay";
	reset-gpio = <&qcom_pinmux 3 GPIO_ACTIVE_LOW>;
	pinctrl-0 = <&pcie0_pins>;
	pinctrl-names = "default";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "pci168c,0040";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_art_6>, <&precal_art_1000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
			mac-address-increment = <(1)>;
		};
	};
};

&pcie1 {
	status = "okay";
	reset-gpio = <&qcom_pinmux 48 GPIO_ACTIVE_LOW>;
	pinctrl-0 = <&pcie1_pins>;
	pinctrl-names = "default";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "pci168c,0040";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_art_6>, <&precal_art_5000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
			mac-address-increment = <(2)>;
		};
	};
};

&nand {
	status = "okay";

	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";

	nand@0 {
		reg = <0>;
		compatible = "qcom,nandcs";

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;
		nand-ecc-step-size = <512>;

		nand-is-boot-medium;
		qcom,boot_pages_size = <0x1180000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			qcadata@0 {
				label = "qcadata";
				reg = <0x0000000 0x0c80000>;
				read-only;
			};

			APPSBL@c80000 {
				label = "APPSBL";
				reg = <0x0c80000 0x0500000>;
				read-only;
			};

			APPSBLENV@1180000 {
				label = "APPSBLENV";
				reg = <0x1180000 0x0080000>;
				read-only;
			};

			art@1200000 {
				label = "art";
				reg = <0x1200000 0x0140000>;
				read-only;
				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_art_0: macaddr@0 {
					reg = <0x0 0x6>;
				};

				macaddr_art_6: macaddr@6 {
					reg = <0x6 0x6>;
				};

				precal_art_1000: precal@1000 {
					reg = <0x1000 0x2f20>;
				};

				precal_art_5000: precal@5000 {
					reg = <0x5000 0x2f20>;
				};
			};

			artbak: art@1340000 {
				label = "artbak";
				reg = <0x1340000 0x0140000>;
				read-only;
			};

			kernel@1480000 {
				label = "kernel";
				reg = <0x1480000 0x0400000>;
			};

			ubi@1880000 {
				label = "ubi";
				reg = <0x1880000 0x6080000>;
			};

			reserve@7900000 {
				label = "reserve";
				reg = <0x7900000 0x0700000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	phy0: ethernet-phy@0 {
		reg = <0>;
		qca,ar8327-initvals = <
			0x00004 0x7600000   /* PAD0_MODE */
			0x00008 0x1000000   /* PAD5_MODE */
			0x0000c 0x80        /* PAD6_MODE */
			0x000e4 0xaa545     /* MAC_POWER_SEL */
			0x000e0 0xc74164de  /* SGMII_CTRL */
			0x0007c 0x4e        /* PORT0_STATUS */
			0x00094 0x4e        /* PORT6_STATUS */
			>;
	};

	phy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <2>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};
