--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -82,6 +82,17 @@ config WS_AP3710I
 	  This board is a Concurrent Dual-Band wireless access point with a
 	  Freescale P1020 SoC.
 
+config WS_AP3715I
+	bool "Enterasys WS-AP3715i"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	help
+	  This option enables support for the Enterasys WS-AP3715i board.
+
+	  This board is a Concurrent Dual-Band wireless access point with a
+	  Freescale P1010 SoC.
+
 config WS_AP3825I
 	bool "Extreme Networks WS-AP3825i"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -27,6 +27,7 @@ obj-$(CONFIG_P1023_RDB)   += p1023_rdb.o
 obj-$(CONFIG_PANDA)       += panda.o
 obj-$(CONFIG_TWR_P102x)   += twr_p102x.o
 obj-$(CONFIG_WS_AP3710I)  += ws-ap3710i.o
+obj-$(CONFIG_WS_AP3715I)  += ws-ap3715i.o
 obj-$(CONFIG_WS_AP3825I)  += ws-ap3825i.o
 obj-$(CONFIG_FIREBOX_T10) += firebox_t10.o
 obj-$(CONFIG_CORENET_GENERIC)   += corenet_generic.o
--- a/arch/powerpc/boot/Makefile
+++ b/arch/powerpc/boot/Makefile
@@ -340,6 +340,7 @@ image-$(CONFIG_TQM8560)			+= cuImage.tqm
 image-$(CONFIG_SBC8548)			+= cuImage.sbc8548
 image-$(CONFIG_KSI8560)			+= cuImage.ksi8560
 image-$(CONFIG_TL_WDR4900_V1)		+= simpleImage.tl-wdr4900-v1
+image-$(CONFIG_WS_AP3715I)		+= simpleImage.ws-ap3715i
 image-$(CONFIG_WS_AP3825I)		+= simpleImage.ws-ap3825i
 # Board ports in arch/powerpc/platform/86xx/Kconfig
 image-$(CONFIG_MVME7100)                += dtbImage.mvme7100
--- a/arch/powerpc/boot/wrapper
+++ b/arch/powerpc/boot/wrapper
@@ -324,6 +324,7 @@ adder875-redboot)
     platformo="$object/fixed-head.o $object/redboot-8xx.o"
     binary=y
     ;;
+simpleboot-ws-ap3715i|\
 simpleboot-ws-ap3825i|\
 simpleboot-tl-wdr4900-v1)
     platformo="$object/fixed-head.o $object/simpleboot.o"
