#include "qcom-ipq8064-eax500.dtsi"

/ {
	model = "Linksys EA8500 WiFi Router";
	compatible = "linksys,ea8500", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		mdio-gpio0 = &mdio0;

		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wifi {
			label = "wifi";
			gpios = <&qcom_pinmux 67 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 68 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		wps {
			label = "green:wps";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
		};

		led_power: power {
			label = "white:power";
			gpios = <&qcom_pinmux 6 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		wifi {
			label = "green:wifi";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_HIGH>;
		};
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio65", "gpio67", "gpio68";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio6", "gpio53", "gpio54";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};
};

&sata_phy {
	status = "okay";
};

&sata {
	status = "okay";
};

&partitions {
	partition@5f80000 {
		label = "syscfg";
		reg = <0x5f80000 0x2080000>;
	};
};

&mdio0 {
	phy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&gmac1 {
	qcom,phy_mdio_addr = <4>;
	qcom,poll_required = <1>;
	qcom,rgmii_delay = <0>;
	qcom,emulation = <0>;
};

/* LAN */
&gmac2 {
	qcom,phy_mdio_addr = <0>;	/* none */
	qcom,poll_required = <0>;	/* no polling */
	qcom,rgmii_delay = <0>;
	qcom,emulation = <0>;
};
