From aae94965421d23e1bf28a5e0180fd698fd3eeb57 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Sat, 19 Mar 2022 22:19:51 +0000
Subject: [PATCH] overlays: Fix cam*_reg_gpio parameter on CM1

See: https://github.com/raspberrypi/linux/pull/4945

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/bcm2708-rpi-cm.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
@@ -15,8 +15,8 @@
 		act_led_activelow = <&act_led>,"gpios:8";
 		act_led_trigger = <&act_led>,"linux,default-trigger";
 		cam0_reg = <&cam0_reg>,"status";
-		cam0_reg_gpio = <&cam0_reg>,"gpios:4";
+		cam0_reg_gpio = <&cam0_reg>,"gpio:4";
 		cam1_reg = <&cam1_reg>,"status";
-		cam1_reg_gpio = <&cam1_reg>,"gpios:4";
+		cam1_reg_gpio = <&cam1_reg>,"gpio:4";
 	};
 };
