From dc01fca5a9d9c09ce9a3fb2bc2e7715c37ff3bd9 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Thu, 1 Apr 2021 14:30:06 +0200
Subject: [PATCH] PCI: aardvark: Don't mask irq when mapping
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

By default, all Legacy INTx interrupts are masked, so there is no need to
mask this interrupt during irq_map callback.

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/pci/controller/pci-aardvark.c | 1 -
 1 file changed, 1 deletion(-)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1339,7 +1339,6 @@ static int advk_pcie_irq_map(struct irq_
 {
 	struct advk_pcie *pcie = h->host_data;
 
-	advk_pcie_irq_mask(irq_get_irq_data(virq));
 	irq_set_status_flags(virq, IRQ_LEVEL);
 	irq_set_chip_and_handler(virq, &pcie->irq_chip,
 				 handle_level_irq);
