From abea9147d22704cdfb68b7161a71dc9fb8fcb0b0 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Noralf=20Tr=C3=B8nnes?= <noralf@tronnes.org>
Date: Fri, 26 Jun 2015 14:25:01 +0200
Subject: [PATCH] firmware: bcm2835: Support ARCH_BCM270x
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Support booting without Device Tree.
Turn on USB power.
Load driver early because of lacking support for deferred probing
in many drivers.

Signed-off-by: Noralf Trønnes <noralf@tronnes.org>

firmware: bcm2835: Don't turn on USB power

The raspberrypi-power driver is now used to turn on USB power.

This partly reverts commit:
firmware: bcm2835: Support ARCH_BCM270x

Signed-off-by: Noralf Trønnes <noralf@tronnes.org>
---
 drivers/firmware/raspberrypi.c | 17 ++++++++++++++++-
 1 file changed, 16 insertions(+), 1 deletion(-)

--- a/drivers/firmware/raspberrypi.c
+++ b/drivers/firmware/raspberrypi.c
@@ -32,6 +32,8 @@ struct rpi_firmware {
 	struct kref consumers;
 };
 
+static struct platform_device *g_pdev;
+
 static DEFINE_MUTEX(transaction_lock);
 
 static void response_callback(struct mbox_client *cl, void *msg)
@@ -280,6 +282,7 @@ static int rpi_firmware_probe(struct pla
 	kref_init(&fw->consumers);
 
 	platform_set_drvdata(pdev, fw);
+	g_pdev = pdev;
 
 	rpi_firmware_print_firmware_revision(fw);
 	rpi_register_hwmon_driver(dev, fw);
@@ -308,6 +311,7 @@ static int rpi_firmware_remove(struct pl
 	rpi_clk = NULL;
 
 	rpi_firmware_put(fw);
+	g_pdev = NULL;
 
 	return 0;
 }
@@ -382,7 +386,18 @@ static struct platform_driver rpi_firmwa
 	.shutdown	= rpi_firmware_shutdown,
 	.remove		= rpi_firmware_remove,
 };
-module_platform_driver(rpi_firmware_driver);
+
+static int __init rpi_firmware_init(void)
+{
+	return platform_driver_register(&rpi_firmware_driver);
+}
+subsys_initcall(rpi_firmware_init);
+
+static void __init rpi_firmware_exit(void)
+{
+	platform_driver_unregister(&rpi_firmware_driver);
+}
+module_exit(rpi_firmware_exit);
 
 MODULE_AUTHOR("Eric Anholt <eric@anholt.net>");
 MODULE_DESCRIPTION("Raspberry Pi firmware driver");
