// SPDX-License-Identifier: GPL-2.0-only
/*
 * Device Tree file for Ubiquiti Nanobeam NBE-5AC-19 (XC)
 *
 * Copyright (C) 2022 Daniel González Cabanelas <dgcbueu@gmail.com>
 * based on device tree from qca9558_ubnt_powerbeam-5ac-500.dts
 */

#include "qca955x_ubnt_xc.dtsi"

/ {
	compatible = "ubnt,nanobeam-ac-xc", "ubnt,xc", "qca,qca9558";
	model = "Ubiquiti NanoBeam AC Gen1 (XC)";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios  = <&gpio 0 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		cs-gpios   = <&gpio 3 GPIO_ACTIVE_HIGH>;
		num-chipselects = <1>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <10000000>;
			enable-gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		rssi0 {
			label = "blue:rssi0";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
		};
		rssi1 {
			label = "blue:rssi1";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
		};
		rssi2 {
			label = "blue:rssi2";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
		};
		rssi3 {
			label = "blue:rssi3";
			gpios = <&led_gpio 3 GPIO_ACTIVE_LOW>;
		};
		led_power: power {
			label = "blue:power";
			gpios = <&led_gpio 4 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		phy-mode = "sgmii";
		reg = <4>;
		at803x-override-sgmii-link-check;
	};
};

&eth0 {
	status = "okay";

	pll-reg = <0 0x48 0>;
	pll-data = <0x03000000 0x00000101 0x00001313>;
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
	phy-mode = "sgmii";
	phy-handle = <&phy4>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
