#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "iodata,wn-ax1167gr", "mediatek,mt7621-soc";
	model = "I-O DATA WN-AX1167GR";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "green:wps";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		auto {
			label = "auto";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		custom {
			label = "custom";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "Bootloader";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "Config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			iNIC_rf: partition@50000 {
				label = "iNIC_rf";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x60000 0xf30000>;
			};

			partition@f90000 {
				label = "Key";
				reg = <0xf90000 0x10000>;
				read-only;
			};

			partition@fa0000 {
				label = "backup";
				reg = <0xfa0000 0x10000>;
				read-only;
			};

			partition@fb0000 {
				label = "storage";
				reg = <0xfb0000 0x50000>;
				read-only;
			};
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_iNIC_rf_4>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy0>;

	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;
};

&mdio {
	ethphy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan4";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};

		port@3 {
			status = "okay";
			label = "lan2";
		};

		port@4 {
			status = "okay";
			label = "lan1";
		};
	};
};

&state_default {
	gpio {
		groups = "uart2", "uart3", "jtag";
		function = "gpio";
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&iNIC_rf 0x0>;
	};
};

&pcie1 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&xhci {
	status = "disabled";
};

&iNIC_rf {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_iNIC_rf_4: macaddr@4 {
		reg = <0x4 0x6>;
	};
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_4: macaddr@4 {
		reg = <0x4 0x6>;
	};
};
