From f5d83b714e304d5f3229da434af2eeea033c4f5d Mon Sep 17 00:00:00 2001
From: William Zhang <william.zhang@broadcom.com>
Date: Mon, 6 Feb 2023 22:58:15 -0800
Subject: [PATCH] arm64: dts: broadcom: bcmbca: Add spi controller node

Add support for HSSPI controller in ARMv8 chip dts files.

Signed-off-by: William Zhang <william.zhang@broadcom.com>
Link: https://lore.kernel.org/r/20230207065826.285013-5-william.zhang@broadcom.com
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 .../boot/dts/broadcom/bcmbca/bcm4908.dtsi     | 18 +++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm4912.dtsi     | 20 +++++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm63146.dtsi    | 19 ++++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm63158.dtsi    | 19 ++++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm6813.dtsi     | 20 +++++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm6856.dtsi     | 18 +++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm6858.dtsi     | 18 +++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm94908.dts     |  4 ++++
 .../boot/dts/broadcom/bcmbca/bcm94912.dts     |  4 ++++
 .../boot/dts/broadcom/bcmbca/bcm963146.dts    |  4 ++++
 .../boot/dts/broadcom/bcmbca/bcm963158.dts    |  4 ++++
 .../boot/dts/broadcom/bcmbca/bcm96813.dts     |  4 ++++
 .../boot/dts/broadcom/bcmbca/bcm96856.dts     |  4 ++++
 .../boot/dts/broadcom/bcmbca/bcm96858.dts     |  4 ++++
 14 files changed, 160 insertions(+)

--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908.dtsi
@@ -107,6 +107,12 @@
 			clock-frequency = <50000000>;
 			clock-output-names = "periph";
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <400000000>;
+		};
 	};
 
 	soc {
@@ -531,6 +537,18 @@
 			#size-cells = <0>;
 		};
 
+		hsspi: spi@1000{
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm4908-hsspi", "brcm,bcmbca-hsspi-v1.0";
+			reg = <0x1000 0x600>;
+			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
+
 		nand-controller@1800 {
 			#address-cells = <1>;
 			#size-cells = <0>;
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm4912.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4912.dtsi
@@ -79,6 +79,7 @@
 			#clock-cells = <0>;
 			clock-frequency = <200000000>;
 		};
+
 		uart_clk: uart-clk {
 			compatible = "fixed-factor-clock";
 			#clock-cells = <0>;
@@ -86,6 +87,12 @@
 			clock-div = <4>;
 			clock-mult = <1>;
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <200000000>;
+		};
 	};
 
 	psci {
@@ -117,6 +124,19 @@
 		#size-cells = <1>;
 		ranges = <0x0 0x0 0xff800000 0x800000>;
 
+		hsspi: spi@1000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm4912-hsspi", "brcm,bcmbca-hsspi-v1.1";
+			reg = <0x1000 0x600>, <0x2610 0x4>;
+			reg-names = "hsspi", "spim-ctrl";
+			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
+
 		uart0: serial@12000 {
 			compatible = "arm,pl011", "arm,primecell";
 			reg = <0x12000 0x1000>;
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm63146.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm63146.dtsi
@@ -60,6 +60,7 @@
 			#clock-cells = <0>;
 			clock-frequency = <200000000>;
 		};
+
 		uart_clk: uart-clk {
 			compatible = "fixed-factor-clock";
 			#clock-cells = <0>;
@@ -67,6 +68,12 @@
 			clock-div = <4>;
 			clock-mult = <1>;
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <200000000>;
+		};
 	};
 
 	psci {
@@ -99,6 +106,18 @@
 		#size-cells = <1>;
 		ranges = <0x0 0x0 0xff800000 0x800000>;
 
+		hsspi: spi@1000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm63146-hsspi", "brcm,bcmbca-hsspi-v1.0";
+			reg = <0x1000 0x600>;
+			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
+
 		uart0: serial@12000 {
 			compatible = "arm,pl011", "arm,primecell";
 			reg = <0x12000 0x1000>;
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm63158.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm63158.dtsi
@@ -79,6 +79,7 @@
 			#clock-cells = <0>;
 			clock-frequency = <200000000>;
 		};
+
 		uart_clk: uart-clk {
 			compatible = "fixed-factor-clock";
 			#clock-cells = <0>;
@@ -86,6 +87,12 @@
 			clock-div = <4>;
 			clock-mult = <1>;
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <400000000>;
+		};
 	};
 
 	psci {
@@ -117,6 +124,18 @@
 		#size-cells = <1>;
 		ranges = <0x0 0x0 0xff800000 0x800000>;
 
+		hsspi: spi@1000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm63158-hsspi", "brcm,bcmbca-hsspi-v1.0";
+			reg = <0x1000 0x600>;
+			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
+
 		uart0: serial@12000 {
 			compatible = "arm,pl011", "arm,primecell";
 			reg = <0x12000 0x1000>;
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm6813.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm6813.dtsi
@@ -79,6 +79,7 @@
 			#clock-cells = <0>;
 			clock-frequency = <200000000>;
 		};
+
 		uart_clk: uart-clk {
 			compatible = "fixed-factor-clock";
 			#clock-cells = <0>;
@@ -86,6 +87,12 @@
 			clock-div = <4>;
 			clock-mult = <1>;
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <200000000>;
+		};
 	};
 
 	psci {
@@ -117,6 +124,19 @@
 		#size-cells = <1>;
 		ranges = <0x0 0x0 0xff800000 0x800000>;
 
+		hsspi: spi@1000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm6813-hsspi", "brcm,bcmbca-hsspi-v1.1";
+			reg = <0x1000 0x600>, <0x2610 0x4>;
+			reg-names = "hsspi", "spim-ctrl";
+			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
+
 		uart0: serial@12000 {
 			compatible = "arm,pl011", "arm,primecell";
 			reg = <0x12000 0x1000>;
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm6856.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm6856.dtsi
@@ -60,6 +60,12 @@
 			#clock-cells = <0>;
 			clock-frequency = <200000000>;
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <400000000>;
+		};
 	};
 
 	psci {
@@ -100,5 +106,17 @@
 			clock-names = "refclk";
 			status = "disabled";
 		};
+
+		hsspi: spi@1000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm6856-hsspi", "brcm,bcmbca-hsspi-v1.0";
+			reg = <0x1000 0x600>;
+			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
 	};
 };
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm6858.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm6858.dtsi
@@ -78,6 +78,12 @@
 			#clock-cells = <0>;
 			clock-frequency = <200000000>;
 		};
+
+		hsspi_pll: hsspi-pll {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <400000000>;
+		};
 	};
 
 	psci {
@@ -137,5 +143,17 @@
 			clock-names = "refclk";
 			status = "disabled";
 		};
+
+		hsspi: spi@1000 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,bcm6858-hsspi", "brcm,bcmbca-hsspi-v1.0";
+			reg = <0x1000 0x600>;
+			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&hsspi_pll &hsspi_pll>;
+			clock-names = "hsspi", "pll";
+			num-cs = <8>;
+			status = "disabled";
+		};
 	};
 };
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm94908.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm94908.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm94912.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm94912.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm963146.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm963146.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm963158.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm963158.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm96813.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm96813.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm96856.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm96856.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm96858.dts
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm96858.dts
@@ -28,3 +28,7 @@
 &uart0 {
 	status = "okay";
 };
+
+&hsspi {
+	status = "okay";
+};
