From 71061acf1a9343317e4d34a2c4578ed9301112cc Mon Sep 17 00:00:00 2001
From: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Date: Wed, 4 May 2022 15:19:17 +0200
Subject: [PATCH] arm64: dts: qcom: ipq8074: add dedicated qcom,ipq8074-dwc3
 compatible

Add dedicated compatible for DWC3 USB node name to allow more accurate
DT schema matching.

Signed-off-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Link: https://lore.kernel.org/r/20220504131923.214367-8-krzysztof.kozlowski@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -554,7 +554,7 @@
 		};
 
 		usb_0: usb@8af8800 {
-			compatible = "qcom,dwc3";
+			compatible = "qcom,ipq8074-dwc3", "qcom,dwc3";
 			reg = <0x08af8800 0x400>;
 			#address-cells = <1>;
 			#size-cells = <1>;
@@ -594,7 +594,7 @@
 		};
 
 		usb_1: usb@8cf8800 {
-			compatible = "qcom,dwc3";
+			compatible = "qcom,ipq8074-dwc3", "qcom,dwc3";
 			reg = <0x08cf8800 0x400>;
 			#address-cells = <1>;
 			#size-cells = <1>;
