// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "glinet,gl-ar750s", "qca,qca9563";
	model = "GL.iNet GL-AR750S";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &eth0;
	};

	keys {
		compatible = "gpio-keys";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		mode {
			label = "mode";
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		led_wlan2g: wlan2g {
			label = "green:wlan2g";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led_wlan5g: wlan5g {
			label = "green:wlan5g";
			gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};
	};

	i2c: i2c {
		compatible = "i2c-gpio";

		sda-gpios = <&gpio  5 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio 21 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>;
	};
};

&spi {
	status = "okay";

	flash_nor: flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		nor_partitions: partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			art: partition@50000 {
				label = "art";
				reg = <0x050000 0x010000>;
				read-only;
			};

			/* Firmware / Kernel flash type specific */
		};
	};

	flash_nand: flash@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <25000000>;

		nand_partitions: partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			nand_ubi: partition@0 {
				label = "nand_ubi";
				reg = <0x000000 0x8000000>;
			};
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&gpio {
	usb_vbus {
		gpio-hog;
		gpios = <7 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "usb-vbus";
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x7c 0x0000007e /* PORT0_STATUS */
		>;
	};
};

&pcie {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb1 {
	status = "okay";
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
