From 349cbe949b9622cc05b148ecfa6268cbbae35b45 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marek=20Beh=C3=BAn?= <kabel@kernel.org>
Date: Mon, 4 Jul 2022 12:59:55 +0200
Subject: [PATCH] leds: turris-omnia: change max brightness from 255 to 1
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Using binary brightness makes more sense for this controller, because
internally in the MCU it works that way: the LED has a color, and a
state whether it is ON or OFF.

The resulting brightness computation with led_mc_calc_color_components()
will now always result in either (0, 0, 0) or the multi_intensity value.

Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/leds/leds-turris-omnia.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/leds/leds-turris-omnia.c
+++ b/drivers/leds/leds-turris-omnia.c
@@ -146,7 +146,7 @@ static int omnia_led_register(struct i2c
 	init_data.fwnode = &np->fwnode;
 
 	cdev = &led->mc_cdev.led_cdev;
-	cdev->max_brightness = 255;
+	cdev->max_brightness = 1;
 	cdev->brightness_set_blocking = omnia_led_brightness_set_blocking;
 	cdev->trigger_type = &omnia_hw_trigger_type;
 	cdev->default_trigger = omnia_hw_trigger.name;
