// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019-orbi.dtsi"

/ {
	model = "NETGEAR SRS60";
	compatible = "netgear,srs60";

	chosen {
		bootargs = "root=/dev/mmcblk0p20 blkdevparts=mmcblk0:512K@17K(0:SBL1)ro,512K(0:BOOTCONFIG)ro,512K(0:QSEE)ro,512K(0:QSEE_1)ro,256K(0:CDT)ro,256K(0:CDT_1)ro,512K(0:BOOTCONFIG1)ro,256K(0:APPSBLENV)ro,1M(0:APPSBL)ro,1M(0:APPSBL_1)ro,256K(0:ART)ro,256K(ARTMTD)ro,2M(language)ro,256K(config)ro,256K(pot)ro,256K(traffic_meter)ro,256K(pot_bak)ro,256K(traffic_meter.bak)ro,3840K(kernel),31488K(rootfs),35328K@9233K(firmware),256K(mtdoops)ro,64K(cert)ro,3840K(kernel-2)ro,31488K(rootfs-2)ro,35328K@44881K(firmware-2)ro,5M(device_table)ro,17M(cp_file)ro,102737K(reserved)ro,-(unallocated) rootfstype=squashfs,ext4 rootwait";
	};
};
