// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcn5502_asus.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	status = "okay";
};
