--- a/arch/arm/boot/dts/marvell/kirkwood-ib62x0.dts
+++ b/arch/arm/boot/dts/marvell/kirkwood-ib62x0.dts
@@ -6,7 +6,14 @@
 
 / {
 	model = "RaidSonic ICY BOX IB-NAS62x0 (Rev B)";
-	compatible = "raidsonic,ib-nas6210-b", "raidsonic,ib-nas6220-b", "raidsonic,ib-nas6210", "raidsonic,ib-nas6220", "raidsonic,ib-nas62x0", "marvell,kirkwood-88f6281", "marvell,kirkwood";
+	compatible = "raidsonic,ib-nas62x0", "marvell,kirkwood-88f6281", "marvell,kirkwood";
+
+	aliases {
+		led-boot = &led_green_os;
+		led-failsafe = &led_red_os;
+		led-running = &led_green_os;
+		led-upgrade = &led_red_os;
+	};
 
 	memory {
 		device_type = "memory";
@@ -81,12 +88,12 @@
 			     &pmx_led_usb_transfer>;
 		pinctrl-names = "default";
 
-		green-os {
+		led_green_os: green-os {
 			label = "ib62x0:green:os";
 			gpios = <&gpio0 25 GPIO_ACTIVE_HIGH>;
-			default-state = "keep";
+			default-state = "on";
 		};
-		red-os {
+		led_red_os: red-os {
 			label = "ib62x0:red:os";
 			gpios = <&gpio0 22 GPIO_ACTIVE_HIGH>;
 		};
@@ -118,13 +125,13 @@
 	};
 
 	partition@100000 {
-		label = "uImage";
-		reg = <0x0100000 0x600000>;
+		label = "second stage u-boot";
+		reg = <0x100000 0x200000>;
 	};
 
-	partition@700000 {
-		label = "root";
-		reg = <0x0700000 0xf900000>;
+	partition@200000 {
+		label = "ubi";
+		reg = <0x200000 0xfe00000>;
 	};
 
 };
