From 1ec26ba377d8ae59cd09811ec78623a750a9c150 Mon Sep 17 00:00:00 2001
From: Hal Feng <hal.feng@starfivetech.com>
Date: Mon, 26 Feb 2024 11:35:44 +0800
Subject: [PATCH 054/116] pinctrl: starfive: jh7110: Unset .strict in
 pinmux_ops

Allow simultaneous use of the same pin for GPIO and another function.
This feature is used in HDMI hot plug detect.

Signed-off-by: Hal Feng <hal.feng@starfivetech.com>
---
 drivers/pinctrl/starfive/pinctrl-starfive-jh7110.c | 1 -
 1 file changed, 1 deletion(-)

--- a/drivers/pinctrl/starfive/pinctrl-starfive-jh7110.c
+++ b/drivers/pinctrl/starfive/pinctrl-starfive-jh7110.c
@@ -327,7 +327,6 @@ static const struct pinmux_ops jh7110_pi
 	.get_function_name   = pinmux_generic_get_function_name,
 	.get_function_groups = pinmux_generic_get_function_groups,
 	.set_mux	     = jh7110_set_mux,
-	.strict		     = true,
 };
 
 static const u8 jh7110_drive_strength_mA[4] = { 2, 4, 8, 12 };
