From effa6ed6ea879ae576a15a063b289d98ae357151 Mon Sep 17 00:00:00 2001
From: Jonathan Bell <jonathan@raspberrypi.org>
Date: Tue, 14 May 2019 17:17:59 +0100
Subject: [PATCH 0159/1085] net: genet: enable link energy detect powerdown for
 external PHYs

There are several warts surrounding bcmgenet_mii_probe() as this
function is called from ndo_open, but it's calling registration-type
functions. The probe should be called at probe time and refactored
such that the PHY device data can be extracted to limit the scope
of this flag to Broadcom PHYs.

For now, pass this flag in as it puts our attached PHY into a low-power
state when disconnected.

Signed-off-by: Jonathan Bell <jonathan@raspberrypi.org>
---
 drivers/net/ethernet/broadcom/genet/bcmmii.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/net/ethernet/broadcom/genet/bcmmii.c
+++ b/drivers/net/ethernet/broadcom/genet/bcmmii.c
@@ -309,6 +309,8 @@ int bcmgenet_mii_probe(struct net_device
 	/* Communicate the integrated PHY revision */
 	if (priv->internal_phy)
 		phy_flags = priv->gphy_rev;
+	else
+		phy_flags = PHY_BRCM_AUTO_PWRDWN_ENABLE;
 
 	/* This is an ugly quirk but we have not been correctly interpreting
 	 * the phy_interface values and we have done that across different
