// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/ {
	/* Lan 49 */
	i2c0: i2c-gpio-0 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 6 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 7 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp0: sfp-p49 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c0>;
		los-gpio = <&gpio1 9 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 8 GPIO_ACTIVE_LOW>;
		/* tx-disable-gpio handled by RTL8214FC based on media setting */
	};

	/* Lan 50 */
	i2c1: i2c-gpio-1 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 1 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 2 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp1: sfp-p50 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c1>;
		los-gpio = <&gpio1 4 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 3 GPIO_ACTIVE_LOW>;
		/* tx-disable-gpio handled by RTL8214FC based on media setting */
	};

	/* Lan 51 */
	i2c2: i2c-gpio-2 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 22 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 23 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp2: sfp-p51 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c2>;
		los-gpio = <&gpio1 25 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 24 GPIO_ACTIVE_LOW>;
		/* tx-disable-gpio handled by RTL8214FC based on media setting */
	};

	/* Lan 52 */
	i2c3: i2c-gpio-3 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 11 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 12 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp3: sfp-p52 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c3>;
		los-gpio = <&gpio1 14 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 13 GPIO_ACTIVE_LOW>;
		/* tx-disable-gpio handled by RTL8214FC based on media setting */
	};
};
