// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/leds/common.h>

#include "mt7628an_xiaomi_mi-router-4.dtsi"

/ {
	compatible = "xiaomi,mi-router-4a-100m", "mediatek,mt7628an-soc";
	model = "Xiaomi Mi Router 4A (100M Edition)";

	aliases {
		led-boot = &led_power_yellow;
		led-failsafe = &led_power_yellow;
		led-running = &led_power_blue;
		led-upgrade = &led_power_yellow;
		label-mac-device = &ethernet;
	};

	leds {
		compatible = "gpio-leds";

		led_power_blue: power_blue {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		led_power_yellow: power_yellow {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_YELLOW>;
			gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};

		wan {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
		};
	};

};

&partitions {
	partition@60000 {
		label = "overlay";
		reg = <0x60000 0x100000>;
		read-only;
	};

	partition@160000 {
		label = "firmware";
		reg = <0x160000 0xea0000>;
		compatible = "denx,uimage";
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_8000>;
		nvmem-cell-names = "eeprom";
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&ethernet {
	nvmem-cells = <&macaddr_factory_4 (-1)>;
	nvmem-cell-names = "mac-address";
};

&esw {
	mediatek,portmap = <0x3e>;
	mediatek,portdisable = <0x2a>;
};
