// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_lan;
		led-failsafe = &led_lan;
		led-upgrade = &led_lan;
		label-mac-device = &eth0;
	};

	leds {
		compatible = "gpio-leds";

		led_lan: lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		wlan5g {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN_5GHZ;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&precal_art_5000>, <&macaddr_info_8>;
		nvmem-cell-names = "pre-calibration", "mac-address";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				label = "partition-table";
				reg = <0x050000 0x010000>;
				read-only;
			};

			partition@60000 {
				label = "info";
				reg = <0x060000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_info_8: macaddr@8 {
						reg = <0x8 0x6>;
					};
				};
			};

			partition@70000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x070000 0xf50000>;
			};

			partition@fc0000 {
				label = "config";
				reg = <0xfc0000 0x030000>;
				read-only;
			};

			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_5000: pre-calibration@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};
};

&pinmux {
	mdio_pins: mdio_pins {
		/* GPIO 10 as MDIO(0x20), GPIO 8 as MDC(0x21) */
		pinctrl-single,bits = <0x8 0x00200021 0x00ff00ff>;
	};
};

&mdio0 {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&mdio_pins>;
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";

	qca956x-serdes-fixup;

	gmac-config {
		device = <&gmac>;
	};
};
