--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -73,6 +73,17 @@ config WS_AP3710I
 	  This board is a Concurrent Dual-Band wireless access point with a
 	  Freescale P1020 SoC.
 
+config WS_AP3715I
+	bool "Enterasys WS-AP3715i"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	help
+	  This option enables support for the Enterasys WS-AP3715i board.
+
+	  This board is a Concurrent Dual-Band wireless access point with a
+	  Freescale P1010 SoC.
+
 config WS_AP3825I
 	bool "Extreme Networks WS-AP3825i"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -26,6 +26,7 @@ obj-$(CONFIG_PANDA)       += panda.o
 obj-$(CONFIG_PPC_P2020)   += p2020.o $(obj8259-y)
 obj-$(CONFIG_TWR_P102x)   += twr_p102x.o
 obj-$(CONFIG_WS_AP3710I)  += ws-ap3710i.o
+obj-$(CONFIG_WS_AP3715I)  += ws-ap3715i.o
 obj-$(CONFIG_WS_AP3825I)  += ws-ap3825i.o
 obj-$(CONFIG_FIREBOX_T10) += firebox_t10.o
 obj-$(CONFIG_CORENET_GENERIC)   += corenet_generic.o
--- a/arch/powerpc/boot/Makefile
+++ b/arch/powerpc/boot/Makefile
@@ -186,6 +186,7 @@ src-plat-$(CONFIG_MVME7100) += motload-h
 src-plat-$(CONFIG_HIVEAP_330) += simpleboot.c fixed-head.S
 src-plat-$(CONFIG_TL_WDR4900_V1) += simpleboot.c fixed-head.S
 src-plat-$(CONFIG_WS_AP3710I) += simpleboot.c fixed-head.S
+src-plat-$(CONFIG_WS_AP3715I) += simpleboot.c fixed-head.S
 src-plat-$(CONFIG_WS_AP3825I) += simpleboot.c fixed-head.S
 
 src-plat-$(CONFIG_PPC_MICROWATT) += fixed-head.S microwatt.c
@@ -361,6 +362,7 @@ image-$(CONFIG_KSI8560)			+= cuImage.ksi
 image-$(CONFIG_HIVEAP_330)		+= simpleImage.hiveap-330
 image-$(CONFIG_TL_WDR4900_V1)		+= simpleImage.tl-wdr4900-v1
 image-$(CONFIG_WS_AP3710I)		+= simpleImage.ws-ap3710i
+image-$(CONFIG_WS_AP3715I)		+= simpleImage.ws-ap3715i
 image-$(CONFIG_WS_AP3825I)		+= simpleImage.ws-ap3825i
 # Board ports in arch/powerpc/platform/86xx/Kconfig
 image-$(CONFIG_MVME7100)                += dtbImage.mvme7100
