From 43d9788f546d24df22d8ba3fcc2497d7ccc198f3 Mon Sep 17 00:00:00 2001
From: Gokul Sriram Palanisamy <gokulsri@codeaurora.org>
Date: Sat, 30 Jan 2021 10:50:11 +0530
Subject: [PATCH] clk: qcom: Add WCSSAON reset

Add WCSSAON reset required for Q6v5 on IPQ8074 SoC.

Signed-off-by: Gokul Sriram Palanisamy <gokulsri@codeaurora.org>
Signed-off-by: Sricharan R <sricharan@codeaurora.org>
Signed-off-by: Nikhil Prakash V <nprakash@codeaurora.org>
Acked-by: Stephen Boyd <sboyd@kernel.org>
---
 drivers/clk/qcom/gcc-ipq8074.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/clk/qcom/gcc-ipq8074.c
+++ b/drivers/clk/qcom/gcc-ipq8074.c
@@ -4712,6 +4712,7 @@ static const struct qcom_reset_map gcc_i
 	[GCC_NSSPORT4_RESET] = { .reg = 0x68014, .bitmask = BIT(27) | GENMASK(9, 8) },
 	[GCC_NSSPORT5_RESET] = { .reg = 0x68014, .bitmask = BIT(28) | GENMASK(11, 10) },
 	[GCC_NSSPORT6_RESET] = { .reg = 0x68014, .bitmask = BIT(29) | GENMASK(13, 12) },
+	[GCC_WCSSAON_RESET] = { 0x59010, 0 },
 };
 
 static struct gdsc *gcc_ipq8074_gdscs[] = {
