// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/* Copyright (c) 2020, Robert Marko <robimarko@gmail.com> */

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Netgear WAC510";
	compatible = "netgear,wac510";

	aliases {
		led-boot = &led_power_amber;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		// TODO: Verify if the ethernet0 alias is needed
		ethernet0 = &gmac;
		ethernet1 = &swport5;
	};

	chosen {
		bootargs-append = " root=/dev/ubiblock0_1";
	};

	soc {
		counter@4a1000 {
			compatible = "qcom,qca-gcnt";
			reg = <0x4a1000 0x4>;
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&tlmm 5 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&tlmm 4 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;

		ssr: ssr@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <1000000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_amber: led-0 {
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_POWER;
			gpios = <&ssr 6 GPIO_ACTIVE_LOW>;
			panic-indicator;
		};

		led_power_green: led-1 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&ssr 5 GPIO_ACTIVE_LOW>;
		};

		led-2 {
			/* 2.4GHz blue - activity */
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <0>;
			gpios = <&ssr 4 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-3 {
			/* 2.4GHz green - link */
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <0>;
			gpios = <&ssr 3 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0radio";
		};

		led-4 {
			/* 5GHz blue - activity */
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <1>;
			gpios = <&ssr 2 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led-5 {
			/* 5GHz green - link */
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <1>;
			gpios = <&ssr 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1radio";
		};

		led-6 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_ACTIVITY;
			gpios = <&ssr 0 GPIO_ACTIVE_LOW>;
		};
	};
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&crypto {
	status = "okay";
};

&tlmm {
	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio53";
			function = "mdio";
			bias-pull-up;
		};

		mux_2 {
			pins = "gpio52";
			function = "mdc";
			bias-pull-up;
		};
	};

	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pinmux {
			function = "blsp_spi0";
			pins = "gpio55", "gpio56", "gpio57";
			drive-strength = <12>;
			bias-disable;
		};

		pinmux_cs {
			function = "gpio";
			pins = "gpio54", "gpio59";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_spi1 {
	status = "okay";

	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>,
		   <&tlmm 59 GPIO_ACTIVE_HIGH>;

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <24000000>;
		reg = <0>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "0:SBL1";
				reg = <0x00000000 0x00040000>;
				read-only;
			};

			partition@40000 {
				label = "0:MIBIB";
				reg = <0x00040000 0x00020000>;
				read-only;
			};

			partition@60000 {
				label = "0:QSEE";
				reg = <0x00060000 0x00060000>;
				read-only;
			};

			partition@c0000 {
				label = "0:CDT";
				reg = <0x000c0000 0x00010000>;
				read-only;
			};

			partition@d0000 {
				label = "0:DDRPARAMS";
				reg = <0x000d0000 0x00010000>;
				read-only;
			};

			partition@e0000 {
				label = "0:APPSBLENV";
				reg = <0x000e0000 0x00010000>;
			};

			partition@f0000 {
				label = "0:APPSBL";
				reg = <0x000f0000 0x000f0000>;
				read-only;
			};

			partition@1e0000 {
				label = "0:MANUDATA";
				reg = <0x001e0000 0x00010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_manudata_6: macaddr@6 {
						compatible = "mac-base";
						reg = <0x6 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@1f0000 {
				label = "0:ART";
				reg = <0x001f0000 0x00010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};

	nand@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "rootfs";
				reg = <0x00000000 0x03800000>;
			};

			partition@3800000 {
				label = "rootfs_1";
				reg = <0x03800000 0x03800000>;
			};

			partition@7000000 {
				label = "var_config";
				reg = <0x07000000 0x00f00000>;
				read-only;
			};

			partition@7f00000 {
				label = "Oops_log";
				reg = <0x07f00000 0x000c0000>;
				read-only;
			};
		};
	};
};

&blsp1_uart1 {
	status = "okay";

	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
};

&cryptobam {
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";

	label = "lan";
};

&swport5 {
	status = "okay";
};

&mdio {
	status = "okay";

	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 62 GPIO_ACTIVE_LOW>;
	reset-delay-us = <2000>;
};

&wifi0 {
	status = "okay";
	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_1000>, <&macaddr_manudata_6 0>;
	qcom,ath10k-calibration-variant = "Netgear-WAC510";
};

&wifi1 {
	status = "okay";
	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_5000>, <&macaddr_manudata_6 16>;
	qcom,ath10k-calibration-variant = "Netgear-WAC510";
};
