From: George Moussalem <george.moussalem@outlook.com>
Date: Wed, 27 Oct 2024 16:34:11 +0400
Subject: [PATCH] wifi: ath11k: update hif and pci ops for QCN6122

Add HIF and PCI ops for QCN6122. QCN6122 by default uses DP window 3.
However, this is configurable, so let's introduce a function to do that and
follow the existing register access code for (hybrid)AHB devices and use 
DP window 1.

Signed-off-by: George Moussalem <george.moussalem@outlook.com>
---
--- a/drivers/net/wireless/ath/ath11k/ahb.c
+++ b/drivers/net/wireless/ath/ath11k/ahb.c
@@ -768,6 +768,18 @@ static int ath11k_ahb_hif_resume(struct
 	return 0;
 }
 
+static void ath11k_ahb_config_static_window_qcn6122(struct ath11k_base *ab)
+{
+	u32 umac_window = FIELD_GET(ATH11K_PCI_WINDOW_VALUE_MASK, HAL_SEQ_WCSS_UMAC_OFFSET);
+	u32 ce_window = FIELD_GET(ATH11K_PCI_WINDOW_VALUE_MASK, HAL_CE_WFSS_CE_REG_BASE);
+	u32 window;
+
+	window = (umac_window) | (ce_window << 6);
+
+	iowrite32(ATH11K_PCI_WINDOW_ENABLE_BIT | window,
+		  ab->mem + ATH11K_PCI_WINDOW_REG_ADDRESS);
+}
+
 static const struct ath11k_hif_ops ath11k_ahb_hif_ops_ipq8074 = {
 	.start = ath11k_ahb_start,
 	.stop = ath11k_ahb_stop,
@@ -800,6 +812,24 @@ static const struct ath11k_hif_ops ath11
 	.ce_irq_disable = ath11k_pci_disable_ce_irqs_except_wake_irq,
 };
 
+static const struct ath11k_hif_ops ath11k_ahb_hif_ops_qcn6122 = {
+	.start = ath11k_pcic_start,
+	.stop = ath11k_pcic_stop,
+	.read32 = ath11k_pcic_read32,
+	.write32 = ath11k_pcic_write32,
+	.read = NULL,
+	.irq_enable = ath11k_pcic_ext_irq_enable,
+	.irq_disable = ath11k_pcic_ext_irq_disable,
+	.get_msi_address =  ath11k_pcic_get_msi_address,
+	.get_user_msi_vector = ath11k_pcic_get_user_msi_assignment,
+	.map_service_to_pipe = ath11k_pcic_map_service_to_pipe,
+	.power_down = ath11k_ahb_power_down,
+	.power_up = ath11k_ahb_power_up,
+	.ce_irq_enable = ath11k_pci_enable_ce_irqs_except_wake_irq,
+	.ce_irq_disable = ath11k_pci_disable_ce_irqs_except_wake_irq,
+	.config_static_window = ath11k_ahb_config_static_window_qcn6122,
+};
+
 static int ath11k_core_get_rproc(struct ath11k_base *ab)
 {
 	struct ath11k_ahb *ab_ahb = ath11k_ahb_priv(ab);
@@ -1144,6 +1174,10 @@ static int ath11k_ahb_probe(struct platf
 		hif_ops = &ath11k_ahb_hif_ops_wcn6750;
 		pci_ops = &ath11k_ahb_pci_ops_wcn6750;
 		break;
+	case ATH11K_HW_QCN6122_HW10:
+		hif_ops = &ath11k_ahb_hif_ops_qcn6122;
+		pci_ops = &ath11k_ahb_pci_ops_wcn6750;
+		break;
 	default:
 		dev_err(&pdev->dev, "unsupported device type %d\n", hw_rev);
 		return -EOPNOTSUPP;
--- a/drivers/net/wireless/ath/ath11k/hif.h
+++ b/drivers/net/wireless/ath/ath11k/hif.h
@@ -32,6 +32,7 @@ struct ath11k_hif_ops {
 	void (*ce_irq_disable)(struct ath11k_base *ab);
 	void (*get_ce_msi_idx)(struct ath11k_base *ab, u32 ce_id, u32 *msi_idx);
 	void (*coredump_download)(struct ath11k_base *ab);
+	void (*config_static_window)(struct ath11k_base *ab);
 };
 
 static inline void ath11k_hif_ce_irq_enable(struct ath11k_base *ab)
@@ -159,4 +160,12 @@ static inline void ath11k_hif_coredump_d
 		ab->hif.ops->coredump_download(ab);
 }
 
+static inline void ath11k_hif_config_static_window(struct ath11k_base *ab)
+{
+	if (!ab->hw_params.static_window_map || !ab->hif.ops->config_static_window)
+		return;
+
+	ab->hif.ops->config_static_window(ab);
+}
+
 #endif /* _HIF_H_ */
--- a/drivers/net/wireless/ath/ath11k/qmi.c
+++ b/drivers/net/wireless/ath/ath11k/qmi.c
@@ -2201,6 +2201,8 @@ static int ath11k_qmi_request_device_inf
 	if (!ab->hw_params.ce_remap)
 		ab->mem_ce = ab->mem;
 
+	ath11k_hif_config_static_window(ab);
+
 	return 0;
 out:
 	return ret;
