From 94800350cb8d2f29dda2206b5e9a3772024ee168 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Thu, 7 Aug 2014 18:30:56 +0200
Subject: [PATCH 08/36] MIPS: lantiq: backport old timer code

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 arch/mips/include/asm/mach-lantiq/lantiq_timer.h |  155 ++++
 arch/mips/lantiq/xway/Makefile                   |    2 +-
 arch/mips/lantiq/xway/timer.c                    |  845 ++++++++++++++++++++++
 3 files changed, 1001 insertions(+), 1 deletion(-)
 create mode 100644 arch/mips/include/asm/mach-lantiq/lantiq_timer.h
 create mode 100644 arch/mips/lantiq/xway/timer.c

--- /dev/null
+++ b/arch/mips/include/asm/mach-lantiq/lantiq_timer.h
@@ -0,0 +1,155 @@
+#ifndef __DANUBE_GPTU_DEV_H__2005_07_26__10_19__
+#define __DANUBE_GPTU_DEV_H__2005_07_26__10_19__
+
+
+/******************************************************************************
+       Copyright (c) 2002, Infineon Technologies.  All rights reserved.
+
+                               No Warranty
+   Because the program is licensed free of charge, there is no warranty for
+   the program, to the extent permitted by applicable law.  Except when
+   otherwise stated in writing the copyright holders and/or other parties
+   provide the program "as is" without warranty of any kind, either
+   expressed or implied, including, but not limited to, the implied
+   warranties of merchantability and fitness for a particular purpose. The
+   entire risk as to the quality and performance of the program is with
+   you.  should the program prove defective, you assume the cost of all
+   necessary servicing, repair or correction.
+
+   In no event unless required by applicable law or agreed to in writing
+   will any copyright holder, or any other party who may modify and/or
+   redistribute the program as permitted above, be liable to you for
+   damages, including any general, special, incidental or consequential
+   damages arising out of the use or inability to use the program
+   (including but not limited to loss of data or data being rendered
+   inaccurate or losses sustained by you or third parties or a failure of
+   the program to operate with any other programs), even if such holder or
+   other party has been advised of the possibility of such damages.
+******************************************************************************/
+
+
+/*
+ * ####################################
+ *              Definition
+ * ####################################
+ */
+
+/*
+ *  Available Timer/Counter Index
+ */
+#define TIMER(n, X)                     (n * 2 + (X ? 1 : 0))
+#define TIMER_ANY                       0x00
+#define TIMER1A                         TIMER(1, 0)
+#define TIMER1B                         TIMER(1, 1)
+#define TIMER2A                         TIMER(2, 0)
+#define TIMER2B                         TIMER(2, 1)
+#define TIMER3A                         TIMER(3, 0)
+#define TIMER3B                         TIMER(3, 1)
+
+/*
+ *  Flag of Timer/Counter
+ *  These flags specify the way in which timer is configured.
+ */
+/*  Bit size of timer/counter.                      */
+#define TIMER_FLAG_16BIT                0x0000
+#define TIMER_FLAG_32BIT                0x0001
+/*  Switch between timer and counter.               */
+#define TIMER_FLAG_TIMER                0x0000
+#define TIMER_FLAG_COUNTER              0x0002
+/*  Stop or continue when overflowing/underflowing. */
+#define TIMER_FLAG_ONCE                 0x0000
+#define TIMER_FLAG_CYCLIC               0x0004
+/*  Count up or counter down.                       */
+#define TIMER_FLAG_UP                   0x0000
+#define TIMER_FLAG_DOWN                 0x0008
+/*  Count on specific level or edge.                */
+#define TIMER_FLAG_HIGH_LEVEL_SENSITIVE 0x0000
+#define TIMER_FLAG_LOW_LEVEL_SENSITIVE  0x0040
+#define TIMER_FLAG_RISE_EDGE            0x0010
+#define TIMER_FLAG_FALL_EDGE            0x0020
+#define TIMER_FLAG_ANY_EDGE             0x0030
+/*  Signal is syncronous to module clock or not.    */
+#define TIMER_FLAG_UNSYNC               0x0000
+#define TIMER_FLAG_SYNC                 0x0080
+/*  Different interrupt handle type.                */
+#define TIMER_FLAG_NO_HANDLE            0x0000
+#if defined(__KERNEL__)
+    #define TIMER_FLAG_CALLBACK_IN_IRQ  0x0100
+#endif  //  defined(__KERNEL__)
+#define TIMER_FLAG_SIGNAL               0x0300
+/*  Internal clock source or external clock source  */
+#define TIMER_FLAG_INT_SRC              0x0000
+#define TIMER_FLAG_EXT_SRC              0x1000
+
+
+/*
+ *  ioctl Command
+ */
+#define GPTU_REQUEST_TIMER              0x01    /*  General method to setup timer/counter.  */
+#define GPTU_FREE_TIMER                 0x02    /*  Free timer/counter.                     */
+#define GPTU_START_TIMER                0x03    /*  Start or resume timer/counter.          */
+#define GPTU_STOP_TIMER                 0x04    /*  Suspend timer/counter.                  */
+#define GPTU_GET_COUNT_VALUE            0x05    /*  Get current count value.                */
+#define GPTU_CALCULATE_DIVIDER          0x06    /*  Calculate timer divider from given freq.*/
+#define GPTU_SET_TIMER                  0x07    /*  Simplified method to setup timer.       */
+#define GPTU_SET_COUNTER                0x08    /*  Simplified method to setup counter.     */
+
+/*
+ *  Data Type Used to Call ioctl
+ */
+struct gptu_ioctl_param {
+    unsigned int                        timer;  /*  In command GPTU_REQUEST_TIMER, GPTU_SET_TIMER, and  *
+                                                 *  GPTU_SET_COUNTER, this field is ID of expected      *
+                                                 *  timer/counter. If it's zero, a timer/counter would  *
+                                                 *  be dynamically allocated and ID would be stored in  *
+                                                 *  this field.                                         *
+                                                 *  In command GPTU_GET_COUNT_VALUE, this field is      *
+                                                 *  ignored.                                            *
+                                                 *  In other command, this field is ID of timer/counter *
+                                                 *  allocated.                                          */
+    unsigned int                        flag;   /*  In command GPTU_REQUEST_TIMER, GPTU_SET_TIMER, and  *
+                                                 *  GPTU_SET_COUNTER, this field contains flags to      *
+                                                 *  specify how to configure timer/counter.             *
+                                                 *  In command GPTU_START_TIMER, zero indicate start    *
+                                                 *  and non-zero indicate resume timer/counter.         *
+                                                 *  In other command, this field is ignored.            */
+    unsigned long                       value;  /*  In command GPTU_REQUEST_TIMER, this field contains  *
+                                                 *  init/reload value.                                  *
+                                                 *  In command GPTU_SET_TIMER, this field contains      *
+                                                 *  frequency (0.001Hz) of timer.                       *
+                                                 *  In command GPTU_GET_COUNT_VALUE, current count      *
+                                                 *  value would be stored in this field.                *
+                                                 *  In command GPTU_CALCULATE_DIVIDER, this field       *
+                                                 *  contains frequency wanted, and after calculation,   *
+                                                 *  divider would be stored in this field to overwrite  *
+                                                 *  the frequency.                                      *
+                                                 *  In other command, this field is ignored.            */
+    int                                 pid;    /*  In command GPTU_REQUEST_TIMER and GPTU_SET_TIMER,   *
+                                                 *  if signal is required, this field contains process  *
+                                                 *  ID to which signal would be sent.                   *
+                                                 *  In other command, this field is ignored.            */
+    int                                 sig;    /*  In command GPTU_REQUEST_TIMER and GPTU_SET_TIMER,   *
+                                                 *  if signal is required, this field contains signal   *
+                                                 *  number which would be sent.                         *
+                                                 *  In other command, this field is ignored.            */
+};
+
+/*
+ * ####################################
+ *              Data Type
+ * ####################################
+ */
+typedef void (*timer_callback)(unsigned long arg);
+
+extern int lq_request_timer(unsigned int, unsigned int, unsigned long, unsigned long, unsigned long);
+extern int lq_free_timer(unsigned int);
+extern int lq_start_timer(unsigned int, int);
+extern int lq_stop_timer(unsigned int);
+extern int lq_reset_counter_flags(u32 timer, u32 flags);
+extern int lq_get_count_value(unsigned int, unsigned long *);
+extern u32 lq_cal_divider(unsigned long);
+extern int lq_set_timer(unsigned int, unsigned int, int, int, unsigned int, unsigned long, unsigned long);
+extern int lq_set_counter(unsigned int timer, unsigned int flag,
+	u32 reload, unsigned long arg1, unsigned long arg2);
+
+#endif /* __DANUBE_GPTU_DEV_H__2005_07_26__10_19__ */
--- a/arch/mips/lantiq/xway/Makefile
+++ b/arch/mips/lantiq/xway/Makefile
@@ -1,4 +1,10 @@
 # SPDX-License-Identifier: GPL-2.0-only
-obj-y := prom.o sysctrl.o clk.o dma.o gptu.o dcdc.o
+obj-y := prom.o sysctrl.o clk.o dma.o dcdc.o
+
+ifdef CONFIG_SOC_AMAZON_SE
+obj-y += gptu.o
+else
+obj-y += timer.o
+endif
 
 obj-y += vmmc.o
--- /dev/null
+++ b/arch/mips/lantiq/xway/timer.c
@@ -0,0 +1,889 @@
+#ifndef CONFIG_SOC_AMAZON_SE
+
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/version.h>
+#include <linux/types.h>
+#include <linux/fs.h>
+#include <linux/miscdevice.h>
+#include <linux/init.h>
+#include <linux/uaccess.h>
+#include <linux/unistd.h>
+#include <linux/errno.h>
+#include <linux/interrupt.h>
+#include <linux/platform_device.h>
+#include <linux/sched.h>
+#include <linux/sched/signal.h>
+
+#include <linux/of_platform.h>
+
+#include <asm/irq.h>
+#include <asm/div64.h>
+#include "../clk.h"
+
+#include <lantiq_soc.h>
+#include <lantiq_irq.h>
+#include <lantiq_timer.h>
+
+#define MAX_NUM_OF_32BIT_TIMER_BLOCKS	6
+
+#ifdef TIMER1A
+#define FIRST_TIMER			TIMER1A
+#else
+#define FIRST_TIMER			2
+#endif
+
+/*
+ *  GPTC divider is set or not.
+ */
+#define GPTU_CLC_RMC_IS_SET		0
+
+/*
+ *  Timer Interrupt (IRQ)
+ */
+/*  Must be adjusted when ICU driver is available */
+#define TIMER_INTERRUPT			(INT_NUM_IM3_IRL0 + 22)
+
+/*
+ *  Bits Operation
+ */
+#define GET_BITS(x, msb, lsb)		\
+	(((x) & ((1 << ((msb) + 1)) - 1)) >> (lsb))
+#define SET_BITS(x, msb, lsb, value)	\
+	(((x) & ~(((1 << ((msb) + 1)) - 1) ^ ((1 << (lsb)) - 1))) | \
+	(((value) & ((1 << (1 + (msb) - (lsb))) - 1)) << (lsb)))
+
+/*
+ *  GPTU Register Mapping
+ */
+#define LQ_GPTU			(KSEG1 + 0x1E100A00)
+#define LQ_GPTU_CLC		((volatile u32 *)(LQ_GPTU + 0x0000))
+#define LQ_GPTU_ID			((volatile u32 *)(LQ_GPTU + 0x0008))
+#define LQ_GPTU_CON(n, X)		((volatile u32 *)(LQ_GPTU + 0x0010 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_RUN(n, X)		((volatile u32 *)(LQ_GPTU + 0x0018 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_RELOAD(n, X)	((volatile u32 *)(LQ_GPTU + 0x0020 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_COUNT(n, X)	((volatile u32 *)(LQ_GPTU + 0x0028 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_IRNEN		((volatile u32 *)(LQ_GPTU + 0x00F4))
+#define LQ_GPTU_IRNICR		((volatile u32 *)(LQ_GPTU + 0x00F8))
+#define LQ_GPTU_IRNCR		((volatile u32 *)(LQ_GPTU + 0x00FC))
+
+/*
+ *  Clock Control Register
+ */
+#define GPTU_CLC_SMC			GET_BITS(*LQ_GPTU_CLC, 23, 16)
+#define GPTU_CLC_RMC			GET_BITS(*LQ_GPTU_CLC, 15, 8)
+#define GPTU_CLC_FSOE			(*LQ_GPTU_CLC & (1 << 5))
+#define GPTU_CLC_EDIS			(*LQ_GPTU_CLC & (1 << 3))
+#define GPTU_CLC_SPEN			(*LQ_GPTU_CLC & (1 << 2))
+#define GPTU_CLC_DISS			(*LQ_GPTU_CLC & (1 << 1))
+#define GPTU_CLC_DISR			(*LQ_GPTU_CLC & (1 << 0))
+
+#define GPTU_CLC_SMC_SET(value)		SET_BITS(0, 23, 16, (value))
+#define GPTU_CLC_RMC_SET(value)		SET_BITS(0, 15, 8, (value))
+#define GPTU_CLC_FSOE_SET(value)	((value) ? (1 << 5) : 0)
+#define GPTU_CLC_SBWE_SET(value)	((value) ? (1 << 4) : 0)
+#define GPTU_CLC_EDIS_SET(value)	((value) ? (1 << 3) : 0)
+#define GPTU_CLC_SPEN_SET(value)	((value) ? (1 << 2) : 0)
+#define GPTU_CLC_DISR_SET(value)	((value) ? (1 << 0) : 0)
+
+/*
+ *  ID Register
+ */
+#define GPTU_ID_ID			GET_BITS(*LQ_GPTU_ID, 15, 8)
+#define GPTU_ID_CFG			GET_BITS(*LQ_GPTU_ID, 7, 5)
+#define GPTU_ID_REV			GET_BITS(*LQ_GPTU_ID, 4, 0)
+
+/*
+ *  Control Register of Timer/Counter nX
+ *    n is the index of block (1 based index)
+ *    X is either A or B
+ */
+#define GPTU_CON_SRC_EG(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 10))
+#define GPTU_CON_SRC_EXT(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 9))
+#define GPTU_CON_SYNC(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 8))
+#define GPTU_CON_EDGE(n, X)		GET_BITS(*LQ_GPTU_CON(n, X), 7, 6)
+#define GPTU_CON_INV(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 5))
+#define GPTU_CON_EXT(n, X)		(*LQ_GPTU_CON(n, A) & (1 << 4))	/* Timer/Counter B does not have this bit */
+#define GPTU_CON_STP(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 3))
+#define GPTU_CON_CNT(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 2))
+#define GPTU_CON_DIR(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 1))
+#define GPTU_CON_EN(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 0))
+
+#define GPTU_CON_SRC_EG_SET(value)	((value) ? 0 : (1 << 10))
+#define GPTU_CON_SRC_EXT_SET(value)	((value) ? (1 << 9) : 0)
+#define GPTU_CON_SYNC_SET(value)	((value) ? (1 << 8) : 0)
+#define GPTU_CON_EDGE_SET(value)	SET_BITS(0, 7, 6, (value))
+#define GPTU_CON_INV_SET(value)		((value) ? (1 << 5) : 0)
+#define GPTU_CON_EXT_SET(value)		((value) ? (1 << 4) : 0)
+#define GPTU_CON_STP_SET(value)		((value) ? (1 << 3) : 0)
+#define GPTU_CON_CNT_SET(value)		((value) ? (1 << 2) : 0)
+#define GPTU_CON_DIR_SET(value)		((value) ? (1 << 1) : 0)
+
+#define GPTU_RUN_RL_SET(value)		((value) ? (1 << 2) : 0)
+#define GPTU_RUN_CEN_SET(value)		((value) ? (1 << 1) : 0)
+#define GPTU_RUN_SEN_SET(value)		((value) ? (1 << 0) : 0)
+
+#define GPTU_IRNEN_TC_SET(n, X, value)	((value) ? (1 << (((n) - 1) * 2 + (X))) : 0)
+#define GPTU_IRNCR_TC_SET(n, X, value)	((value) ? (1 << (((n) - 1) * 2 + (X))) : 0)
+
+#define TIMER_FLAG_MASK_SIZE(x)		(x & 0x0001)
+#define TIMER_FLAG_MASK_TYPE(x)		(x & 0x0002)
+#define TIMER_FLAG_MASK_STOP(x)		(x & 0x0004)
+#define TIMER_FLAG_MASK_DIR(x)		(x & 0x0008)
+#define TIMER_FLAG_NONE_EDGE		0x0000
+#define TIMER_FLAG_MASK_EDGE(x)		(x & 0x0030)
+#define TIMER_FLAG_REAL			0x0000
+#define TIMER_FLAG_INVERT		0x0040
+#define TIMER_FLAG_MASK_INVERT(x)	(x & 0x0040)
+#define TIMER_FLAG_MASK_TRIGGER(x)	(x & 0x0070)
+#define TIMER_FLAG_MASK_SYNC(x)		(x & 0x0080)
+#define TIMER_FLAG_CALLBACK_IN_HB	0x0200
+#define TIMER_FLAG_MASK_HANDLE(x)	(x & 0x0300)
+#define TIMER_FLAG_MASK_SRC(x)		(x & 0x1000)
+
+struct timer_dev_timer {
+	unsigned int f_irq_on;
+	unsigned int irq;
+	unsigned int flag;
+	unsigned long arg1;
+	unsigned long arg2;
+};
+
+struct timer_dev {
+	struct mutex gptu_mutex;
+	unsigned int number_of_timers;
+	unsigned int occupation;
+	unsigned int f_gptu_on;
+	struct timer_dev_timer timer[MAX_NUM_OF_32BIT_TIMER_BLOCKS * 2];
+};
+
+
+static unsigned int ltq_get_fpi_bus_clock(int fpi) {
+	struct clk *clk = clk_get_fpi();
+	return clk_get_rate(clk);
+}
+
+
+static long gptu_ioctl(struct file *, unsigned int, unsigned long);
+static int gptu_open(struct inode *, struct file *);
+static int gptu_release(struct inode *, struct file *);
+
+static struct file_operations gptu_fops = {
+	.owner = THIS_MODULE,
+	.unlocked_ioctl = gptu_ioctl,
+	.open = gptu_open,
+	.release = gptu_release
+};
+
+static struct miscdevice gptu_miscdev = {
+	.minor = MISC_DYNAMIC_MINOR,
+	.name = "gptu",
+	.fops = &gptu_fops,
+};
+
+static struct timer_dev timer_dev;
+
+static irqreturn_t timer_irq_handler(int irq, void *p)
+{
+	unsigned int timer;
+	unsigned int flag;
+	struct timer_dev_timer *dev_timer = (struct timer_dev_timer *)p;
+
+	timer = irq - TIMER_INTERRUPT;
+	if (timer < timer_dev.number_of_timers
+		&& dev_timer == &timer_dev.timer[timer]) {
+		/*  Clear interrupt.    */
+		ltq_w32(1 << timer, LQ_GPTU_IRNCR);
+
+		/*  Call user hanler or signal. */
+		flag = dev_timer->flag;
+		if (!(timer & 0x01)
+			|| TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT) {
+			/* 16-bit timer or timer A of 32-bit timer  */
+			switch (TIMER_FLAG_MASK_HANDLE(flag)) {
+			case TIMER_FLAG_CALLBACK_IN_IRQ:
+			case TIMER_FLAG_CALLBACK_IN_HB:
+				if (dev_timer->arg1)
+					(*(timer_callback)dev_timer->arg1)(dev_timer->arg2);
+				break;
+			case TIMER_FLAG_SIGNAL:
+				send_sig((int)dev_timer->arg2, (struct task_struct *)dev_timer->arg1, 0);
+				break;
+			}
+		}
+	}
+	return IRQ_HANDLED;
+}
+
+static inline void lq_enable_gptu(void)
+{
+	struct clk *clk = clk_get_sys("1e100a00.gptu", NULL);
+	clk_enable(clk);
+
+	//ltq_pmu_enable(PMU_GPT);
+
+	/*  Set divider as 1, disable write protection for SPEN, enable module. */
+	*LQ_GPTU_CLC =
+		GPTU_CLC_SMC_SET(0x00) |
+		GPTU_CLC_RMC_SET(0x01) |
+		GPTU_CLC_FSOE_SET(0) |
+		GPTU_CLC_SBWE_SET(1) |
+		GPTU_CLC_EDIS_SET(0) |
+		GPTU_CLC_SPEN_SET(0) |
+		GPTU_CLC_DISR_SET(0);
+}
+
+static inline void lq_disable_gptu(void)
+{
+	struct clk *clk = clk_get_sys("1e100a00.gptu", NULL);
+	ltq_w32(0x00, LQ_GPTU_IRNEN);
+	ltq_w32(0xfff, LQ_GPTU_IRNCR);
+
+	/*  Set divider as 0, enable write protection for SPEN, disable module. */
+	*LQ_GPTU_CLC =
+		GPTU_CLC_SMC_SET(0x00) |
+		GPTU_CLC_RMC_SET(0x00) |
+		GPTU_CLC_FSOE_SET(0) |
+		GPTU_CLC_SBWE_SET(0) |
+		GPTU_CLC_EDIS_SET(0) |
+		GPTU_CLC_SPEN_SET(0) |
+		GPTU_CLC_DISR_SET(1);
+
+	clk_enable(clk);
+}
+
+int lq_request_timer(unsigned int timer, unsigned int flag,
+	unsigned long value, unsigned long arg1, unsigned long arg2)
+{
+	int ret = 0;
+	unsigned int con_reg, irnen_reg;
+	int n, X;
+
+	if (timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	printk(KERN_INFO "request_timer(%d, 0x%08X, %lu)...",
+		timer, flag, value);
+
+	if (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT)
+		value &= 0xFFFF;
+	else
+		timer &= ~0x01;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	/*
+	 *  Allocate timer.
+	 */
+	if (timer < FIRST_TIMER) {
+		unsigned int mask;
+		unsigned int shift;
+		/* This takes care of TIMER1B which is the only choice for Voice TAPI system */
+		unsigned int offset = TIMER2A;
+
+		/*
+		 *  Pick up a free timer.
+		 */
+		if (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT) {
+			mask = 1 << offset;
+			shift = 1;
+		} else {
+			mask = 3 << offset;
+			shift = 2;
+		}
+		for (timer = offset;
+		     timer < offset + timer_dev.number_of_timers;
+		     timer += shift, mask <<= shift)
+			if (!(timer_dev.occupation & mask)) {
+				timer_dev.occupation |= mask;
+				break;
+			}
+		if (timer >= offset + timer_dev.number_of_timers) {
+			printk("failed![%d]\n", __LINE__);
+			mutex_unlock(&timer_dev.gptu_mutex);
+			return -EINVAL;
+		} else
+			ret = timer;
+	} else {
+		register unsigned int mask;
+
+		/*
+		 *  Check if the requested timer is free.
+		 */
+		mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+		if ((timer_dev.occupation & mask)) {
+			printk("failed![%d] mask %#x, timer_dev.occupation %#x\n",
+				__LINE__, mask, timer_dev.occupation);
+			mutex_unlock(&timer_dev.gptu_mutex);
+			return -EBUSY;
+		} else {
+			timer_dev.occupation |= mask;
+			ret = 0;
+		}
+	}
+
+	/*
+	 *  Prepare control register value.
+	 */
+	switch (TIMER_FLAG_MASK_EDGE(flag)) {
+	default:
+	case TIMER_FLAG_NONE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x00);
+		break;
+	case TIMER_FLAG_RISE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x01);
+		break;
+	case TIMER_FLAG_FALL_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x02);
+		break;
+	case TIMER_FLAG_ANY_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x03);
+		break;
+	}
+	if (TIMER_FLAG_MASK_TYPE(flag) == TIMER_FLAG_TIMER)
+		con_reg |=
+			TIMER_FLAG_MASK_SRC(flag) ==
+			TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EXT_SET(1) :
+			GPTU_CON_SRC_EXT_SET(0);
+	else
+		con_reg |=
+			TIMER_FLAG_MASK_SRC(flag) ==
+			TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EG_SET(1) :
+			GPTU_CON_SRC_EG_SET(0);
+	con_reg |=
+		TIMER_FLAG_MASK_SYNC(flag) ==
+		TIMER_FLAG_UNSYNC ? GPTU_CON_SYNC_SET(0) :
+		GPTU_CON_SYNC_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_INVERT(flag) ==
+		TIMER_FLAG_REAL ? GPTU_CON_INV_SET(0) : GPTU_CON_INV_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_SIZE(flag) ==
+		TIMER_FLAG_16BIT ? GPTU_CON_EXT_SET(0) :
+		GPTU_CON_EXT_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_STOP(flag) ==
+		TIMER_FLAG_ONCE ? GPTU_CON_STP_SET(1) : GPTU_CON_STP_SET(0);
+	con_reg |=
+		TIMER_FLAG_MASK_TYPE(flag) ==
+		TIMER_FLAG_TIMER ? GPTU_CON_CNT_SET(0) :
+		GPTU_CON_CNT_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_DIR(flag) ==
+		TIMER_FLAG_UP ? GPTU_CON_DIR_SET(1) : GPTU_CON_DIR_SET(0);
+
+	/*
+	 *  Fill up running data.
+	 */
+	timer_dev.timer[timer - FIRST_TIMER].flag = flag;
+	timer_dev.timer[timer - FIRST_TIMER].arg1 = arg1;
+	timer_dev.timer[timer - FIRST_TIMER].arg2 = arg2;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer_dev.timer[timer - FIRST_TIMER + 1].flag = flag;
+
+	/*
+	 *  Enable GPTU module.
+	 */
+	if (!timer_dev.f_gptu_on) {
+		lq_enable_gptu();
+		timer_dev.f_gptu_on = 1;
+	}
+
+	/*
+	 *  Enable IRQ.
+	 */
+	if (TIMER_FLAG_MASK_HANDLE(flag) != TIMER_FLAG_NO_HANDLE) {
+		if (TIMER_FLAG_MASK_HANDLE(flag) == TIMER_FLAG_SIGNAL)
+			timer_dev.timer[timer - FIRST_TIMER].arg1 =
+				(unsigned long) find_task_by_vpid((int) arg1);
+
+		irnen_reg = 1 << (timer - FIRST_TIMER);
+
+		if (TIMER_FLAG_MASK_HANDLE(flag) == TIMER_FLAG_SIGNAL
+		    || (TIMER_FLAG_MASK_HANDLE(flag) ==
+			TIMER_FLAG_CALLBACK_IN_IRQ
+			&& timer_dev.timer[timer - FIRST_TIMER].arg1)) {
+			enable_irq(timer_dev.timer[timer - FIRST_TIMER].irq);
+			timer_dev.timer[timer - FIRST_TIMER].f_irq_on = 1;
+		}
+	} else
+		irnen_reg = 0;
+
+	/*
+	 *  Write config register, reload value and enable interrupt.
+	 */
+	n = timer >> 1;
+	X = timer & 0x01;
+	*LQ_GPTU_CON(n, X) = con_reg;
+	*LQ_GPTU_RELOAD(n, X) = value;
+	/* printk("reload value = %d\n", (u32)value); */
+	*LQ_GPTU_IRNEN |= irnen_reg;
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+	printk("successful!\n");
+	return ret;
+}
+EXPORT_SYMBOL(lq_request_timer);
+
+int lq_free_timer(unsigned int timer)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	if (GPTU_CON_EN(n, X))
+		*LQ_GPTU_RUN(n, X) = GPTU_RUN_CEN_SET(1);
+
+	*LQ_GPTU_IRNEN &= ~GPTU_IRNEN_TC_SET(n, X, 1);
+	*LQ_GPTU_IRNCR |= GPTU_IRNCR_TC_SET(n, X, 1);
+
+	if (timer_dev.timer[timer - FIRST_TIMER].f_irq_on) {
+		disable_irq(timer_dev.timer[timer - FIRST_TIMER].irq);
+		timer_dev.timer[timer - FIRST_TIMER].f_irq_on = 0;
+	}
+
+	timer_dev.occupation &= ~mask;
+	if (!timer_dev.occupation && timer_dev.f_gptu_on) {
+		lq_disable_gptu();
+		timer_dev.f_gptu_on = 0;
+	}
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_free_timer);
+
+int lq_start_timer(unsigned int timer, int is_resume)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) ==
+	TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*LQ_GPTU_RUN(n, X) = GPTU_RUN_RL_SET(!is_resume) | GPTU_RUN_SEN_SET(1);
+
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_start_timer);
+
+int lq_stop_timer(unsigned int timer)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER
+	    || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*LQ_GPTU_RUN(n, X) = GPTU_RUN_CEN_SET(1);
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_stop_timer);
+
+int lq_reset_counter_flags(u32 timer, u32 flags)
+{
+	unsigned int oflag;
+	unsigned int mask, con_reg;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	oflag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(oflag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(oflag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	switch (TIMER_FLAG_MASK_EDGE(flags)) {
+	default:
+	case TIMER_FLAG_NONE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x00);
+		break;
+	case TIMER_FLAG_RISE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x01);
+		break;
+	case TIMER_FLAG_FALL_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x02);
+		break;
+	case TIMER_FLAG_ANY_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x03);
+		break;
+	}
+	if (TIMER_FLAG_MASK_TYPE(flags) == TIMER_FLAG_TIMER)
+		con_reg |= TIMER_FLAG_MASK_SRC(flags) == TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EXT_SET(1) : GPTU_CON_SRC_EXT_SET(0);
+	else
+		con_reg |= TIMER_FLAG_MASK_SRC(flags) == TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EG_SET(1) : GPTU_CON_SRC_EG_SET(0);
+	con_reg |= TIMER_FLAG_MASK_SYNC(flags) == TIMER_FLAG_UNSYNC ? GPTU_CON_SYNC_SET(0) : GPTU_CON_SYNC_SET(1);
+	con_reg |= TIMER_FLAG_MASK_INVERT(flags) == TIMER_FLAG_REAL ? GPTU_CON_INV_SET(0) : GPTU_CON_INV_SET(1);
+	con_reg |= TIMER_FLAG_MASK_SIZE(flags) == TIMER_FLAG_16BIT ? GPTU_CON_EXT_SET(0) : GPTU_CON_EXT_SET(1);
+	con_reg |= TIMER_FLAG_MASK_STOP(flags) == TIMER_FLAG_ONCE ? GPTU_CON_STP_SET(1) : GPTU_CON_STP_SET(0);
+	con_reg |= TIMER_FLAG_MASK_TYPE(flags) == TIMER_FLAG_TIMER ? GPTU_CON_CNT_SET(0) : GPTU_CON_CNT_SET(1);
+	con_reg |= TIMER_FLAG_MASK_DIR(flags) == TIMER_FLAG_UP ? GPTU_CON_DIR_SET(1) : GPTU_CON_DIR_SET(0);
+
+	timer_dev.timer[timer - FIRST_TIMER].flag = flags;
+	if (TIMER_FLAG_MASK_SIZE(flags) != TIMER_FLAG_16BIT)
+		timer_dev.timer[timer - FIRST_TIMER + 1].flag = flags;
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*LQ_GPTU_CON(n, X) = con_reg;
+	smp_wmb();
+	mutex_unlock(&timer_dev.gptu_mutex);
+	return 0;
+}
+EXPORT_SYMBOL(lq_reset_counter_flags);
+
+int lq_get_count_value(unsigned int timer, unsigned long *value)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER
+	    || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*value = *LQ_GPTU_COUNT(n, X);
+
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_get_count_value);
+
+u32 lq_cal_divider(unsigned long freq)
+{
+	u64 module_freq, fpi = ltq_get_fpi_bus_clock(2);
+	u32 clock_divider = 1;
+	module_freq = fpi * 1000;
+	do_div(module_freq, clock_divider * freq);
+	return module_freq;
+}
+EXPORT_SYMBOL(lq_cal_divider);
+
+int lq_set_timer(unsigned int timer, unsigned int freq, int is_cyclic,
+	int is_ext_src, unsigned int handle_flag, unsigned long arg1,
+	unsigned long arg2)
+{
+	unsigned long divider;
+	unsigned int flag;
+
+	divider = lq_cal_divider(freq);
+	if (divider == 0)
+		return -EINVAL;
+	flag = ((divider & ~0xFFFF) ? TIMER_FLAG_32BIT : TIMER_FLAG_16BIT)
+		| (is_cyclic ? TIMER_FLAG_CYCLIC : TIMER_FLAG_ONCE)
+		| (is_ext_src ? TIMER_FLAG_EXT_SRC : TIMER_FLAG_INT_SRC)
+		| TIMER_FLAG_TIMER | TIMER_FLAG_DOWN
+		| TIMER_FLAG_MASK_HANDLE(handle_flag);
+
+	printk(KERN_INFO "lq_set_timer(%d, %d), divider = %lu\n",
+		timer, freq, divider);
+	return lq_request_timer(timer, flag, divider, arg1, arg2);
+}
+EXPORT_SYMBOL(lq_set_timer);
+
+int lq_set_counter(unsigned int timer, unsigned int flag, u32 reload,
+	unsigned long arg1, unsigned long arg2)
+{
+	printk(KERN_INFO "lq_set_counter(%d, %#x, %d)\n", timer, flag, reload);
+	return lq_request_timer(timer, flag, reload, arg1, arg2);
+}
+EXPORT_SYMBOL(lq_set_counter);
+
+static long gptu_ioctl(struct file *file, unsigned int cmd,
+	unsigned long arg)
+{
+	int ret;
+	struct gptu_ioctl_param param;
+
+	if (!access_ok((void __user *)arg, sizeof(struct gptu_ioctl_param)))
+		return -EFAULT;
+	if (copy_from_user(&param, (void __user *)arg, sizeof(param)))
+		return -EFAULT;
+
+	if ((((cmd == GPTU_REQUEST_TIMER || cmd == GPTU_SET_TIMER
+	       || GPTU_SET_COUNTER) && param.timer < 2)
+	     || cmd == GPTU_GET_COUNT_VALUE || cmd == GPTU_CALCULATE_DIVIDER)
+	    && !access_ok((void __user *)arg,
+			   sizeof(struct gptu_ioctl_param)))
+		return -EFAULT;
+
+	switch (cmd) {
+	case GPTU_REQUEST_TIMER:
+		ret = lq_request_timer(param.timer, param.flag, param.value,
+				     (unsigned long) param.pid,
+				     (unsigned long) param.sig);
+		if (ret > 0) {
+			if (copy_to_user(&((struct gptu_ioctl_param *) arg)->
+					 timer, &ret, sizeof(&ret)))
+				ret = -EFAULT;
+			else
+				ret = 0;
+		}
+		break;
+	case GPTU_FREE_TIMER:
+		ret = lq_free_timer(param.timer);
+		break;
+	case GPTU_START_TIMER:
+		ret = lq_start_timer(param.timer, param.flag);
+		break;
+	case GPTU_STOP_TIMER:
+		ret = lq_stop_timer(param.timer);
+		break;
+	case GPTU_GET_COUNT_VALUE:
+		ret = lq_get_count_value(param.timer, &param.value);
+		if (!ret && copy_to_user(&((struct gptu_ioctl_param *) arg)->
+		    value, &param.value,sizeof(param.value)))
+			ret = -EFAULT;
+		break;
+	case GPTU_CALCULATE_DIVIDER:
+		param.value = lq_cal_divider(param.value);
+		if (param.value == 0)
+			ret = -EINVAL;
+		else if (copy_to_user(&((struct gptu_ioctl_param *) arg)->
+				      value, &param.value,
+				      sizeof(param.value)))
+			ret = -EFAULT;
+		else
+			ret = 0;
+		break;
+	case GPTU_SET_TIMER:
+		ret = lq_set_timer(param.timer, param.value,
+				 TIMER_FLAG_MASK_STOP(param.flag) !=
+				 TIMER_FLAG_ONCE ? 1 : 0,
+				 TIMER_FLAG_MASK_SRC(param.flag) ==
+				 TIMER_FLAG_EXT_SRC ? 1 : 0,
+				 TIMER_FLAG_MASK_HANDLE(param.flag) ==
+				 TIMER_FLAG_SIGNAL ? TIMER_FLAG_SIGNAL :
+				 TIMER_FLAG_NO_HANDLE,
+				 (unsigned long) param.pid,
+				 (unsigned long) param.sig);
+		if (ret > 0) {
+			if (copy_to_user(&((struct gptu_ioctl_param *) arg)->
+					 timer, &ret, sizeof(&ret)))
+				ret = -EFAULT;
+			else
+				ret = 0;
+		}
+		break;
+	case GPTU_SET_COUNTER:
+		lq_set_counter(param.timer, param.flag, param.value, 0, 0);
+		if (ret > 0) {
+			if (copy_to_user(&((struct gptu_ioctl_param *) arg)->
+					 timer, &ret, sizeof(&ret)))
+				ret = -EFAULT;
+			else
+				ret = 0;
+		}
+		break;
+	default:
+		ret = -ENOTTY;
+	}
+
+	return ret;
+}
+
+static int gptu_open(struct inode *inode, struct file *file)
+{
+	return 0;
+}
+
+static int gptu_release(struct inode *inode, struct file *file)
+{
+	return 0;
+}
+
+static int gptu_probe(struct platform_device *pdev)
+{
+	int ret;
+	int i;
+
+	ltq_w32(0, LQ_GPTU_IRNEN);
+	ltq_w32(0xfff, LQ_GPTU_IRNCR);
+
+	memset(&timer_dev, 0, sizeof(timer_dev));
+	ret = devm_mutex_init(&pdev->dev, &timer_dev.gptu_mutex);
+	if (ret)
+		return ret;
+
+	lq_enable_gptu();
+	timer_dev.number_of_timers = GPTU_ID_CFG * 2;
+	lq_disable_gptu();
+	if (timer_dev.number_of_timers > MAX_NUM_OF_32BIT_TIMER_BLOCKS * 2)
+		timer_dev.number_of_timers = MAX_NUM_OF_32BIT_TIMER_BLOCKS * 2;
+	printk(KERN_INFO "gptu: totally %d 16-bit timers/counters\n", timer_dev.number_of_timers);
+
+	ret = misc_register(&gptu_miscdev);
+	if (ret) {
+		printk(KERN_ERR "gptu: can't misc_register, get error %d\n", -ret);
+		return ret;
+	} else {
+		printk(KERN_INFO "gptu: misc_register on minor %d\n", gptu_miscdev.minor);
+	}
+
+	for (i = 0; i < timer_dev.number_of_timers; i++) {
+		int irq = platform_get_irq(pdev, i);
+		if (irq < 0) {
+			printk(KERN_ERR "gptu: failed in getting irq (%d), get error %d\n", i, irq);
+			for (i--; i >= 0; i--)
+				free_irq(timer_dev.timer[i].irq, &timer_dev.timer[i]);
+			misc_deregister(&gptu_miscdev);
+			return irq;
+		}
+
+		ret = request_irq(irq, timer_irq_handler, IRQF_TIMER, gptu_miscdev.name, &timer_dev.timer[i]);
+		if (ret) {
+			printk(KERN_ERR "gptu: failed in requesting irq (%d), get error %d\n", i, -ret);
+			for (i--; i >= 0; i--)
+				free_irq(timer_dev.timer[i].irq, &timer_dev.timer[i]);
+			misc_deregister(&gptu_miscdev);
+			return ret;
+		} else {
+			timer_dev.timer[i].irq = irq;
+			disable_irq(timer_dev.timer[i].irq);
+			printk(KERN_INFO "gptu: succeeded to request irq %d\n", timer_dev.timer[i].irq);
+		}
+	}
+
+	return 0;
+}
+
+static const struct of_device_id gptu_match[] = {
+	{ .compatible = "lantiq,gptu-xway" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, gptu_match);
+
+static struct platform_driver gptu_driver = {
+	.probe = gptu_probe,
+	.driver = {
+		.name = "gptu-xway",
+		.of_match_table = gptu_match,
+	},
+};
+
+static int __init lq_gptu_init(void)
+{
+	int ret = platform_driver_register(&gptu_driver);
+
+	if (ret)
+		pr_info("gptu: Error registering platform driver\n");
+	return ret;
+}
+
+static void __exit lq_gptu_exit(void)
+{
+	unsigned int i;
+
+	for (i = 0; i < timer_dev.number_of_timers; i++) {
+		if (timer_dev.timer[i].f_irq_on)
+			disable_irq(timer_dev.timer[i].irq);
+		free_irq(timer_dev.timer[i].irq, &timer_dev.timer[i]);
+	}
+	lq_disable_gptu();
+	misc_deregister(&gptu_miscdev);
+}
+
+module_init(lq_gptu_init);
+module_exit(lq_gptu_exit);
+
+#endif
