From 8c73af6e8d78c66cfef0f551b00d375ec0b67ff3 Mon Sep 17 00:00:00 2001
From: Gokul Sriram Palanisamy <gokulsri@codeaurora.org>
Date: Sat, 30 Jan 2021 10:50:09 +0530
Subject: [PATCH] remoteproc: qcom: Update regmap offsets for halt register

Fixed issue in reading halt-regs parameter from device-tree.

Signed-off-by: Gokul Sriram Palanisamy <gokulsri@codeaurora.org>
Signed-off-by: Sricharan R <sricharan@codeaurora.org>
---
 drivers/remoteproc/qcom_q6v5_wcss.c | 22 ++++++++++++++--------
 1 file changed, 14 insertions(+), 8 deletions(-)

--- a/drivers/remoteproc/qcom_q6v5_wcss.c
+++ b/drivers/remoteproc/qcom_q6v5_wcss.c
@@ -86,7 +86,7 @@
 #define TCSR_WCSS_CLK_MASK	0x1F
 #define TCSR_WCSS_CLK_ENABLE	0x14
 
-#define MAX_HALT_REG		3
+#define MAX_HALT_REG		4
 
 #define WCNSS_PAS_ID		6
 
@@ -155,6 +155,7 @@ struct wcss_data {
 	u32 version;
 	bool aon_reset_required;
 	bool wcss_q6_reset_required;
+	bool bcr_reset_required;
 	const char *ssr_name;
 	const char *sysmon_name;
 	int ssctl_id;
@@ -876,10 +877,13 @@ static int q6v5_wcss_init_reset(struct q
 		}
 	}
 
-	wcss->wcss_q6_bcr_reset = devm_reset_control_get_exclusive(dev, "wcss_q6_bcr_reset");
-	if (IS_ERR(wcss->wcss_q6_bcr_reset)) {
-		dev_err(wcss->dev, "unable to acquire wcss_q6_bcr_reset\n");
-		return PTR_ERR(wcss->wcss_q6_bcr_reset);
+	if (desc->bcr_reset_required) {
+		wcss->wcss_q6_bcr_reset = devm_reset_control_get_exclusive(dev,
+									   "wcss_q6_bcr_reset");
+		if (IS_ERR(wcss->wcss_q6_bcr_reset)) {
+			dev_err(wcss->dev, "unable to acquire wcss_q6_bcr_reset\n");
+			return PTR_ERR(wcss->wcss_q6_bcr_reset);
+		}
 	}
 
 	return 0;
@@ -929,9 +933,9 @@ static int q6v5_wcss_init_mmio(struct q6
 		return -EINVAL;
 	}
 
-	wcss->halt_q6 = halt_reg[0];
-	wcss->halt_wcss = halt_reg[1];
-	wcss->halt_nc = halt_reg[2];
+	wcss->halt_q6 = halt_reg[1];
+	wcss->halt_wcss = halt_reg[2];
+	wcss->halt_nc = halt_reg[3];
 
 	return 0;
 }
@@ -1173,6 +1177,7 @@ static const struct wcss_data wcss_ipq80
 	.crash_reason_smem = WCSS_CRASH_REASON,
 	.aon_reset_required = true,
 	.wcss_q6_reset_required = true,
+	.bcr_reset_required = false,
 	.ssr_name = "q6wcss",
 	.ops = &q6v5_wcss_ipq8074_ops,
 	.requires_force_stop = true,
@@ -1187,6 +1192,7 @@ static const struct wcss_data wcss_qcs40
 	.version = WCSS_QCS404,
 	.aon_reset_required = false,
 	.wcss_q6_reset_required = false,
+	.bcr_reset_required = true,
 	.ssr_name = "mpss",
 	.sysmon_name = "wcnss",
 	.ssctl_id = 0x12,
