// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "YYeTs LE1";
	compatible = "yyets,le1";

	aliases {
		led-boot = &led_usb;
		led-failsafe = &led_usb;
		led-upgrade = &led_usb;

		ethernet0 = &swport5;
		ethernet1 = &gmac;
		label-mac-device = &gmac;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_usb: usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 36 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "usbport";
			trigger-sources = <&usb3_port1>, <&usb3_port2>, <&usb2_port1>;
		};

		wlan2g {
			label = "green:wlan2g";
			gpios = <&tlmm 32 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "green:wlan5g";
			gpios = <&tlmm 50 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	soc {
		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_spi1 {
	cs-gpios = <&tlmm 12 GPIO_ACTIVE_LOW>;
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "MIBIB";
				reg = <0x40000 0x20000>;
				read-only;
			};

			partition@60000 {
				label = "QSEE";
				reg = <0x60000 0x60000>;
				read-only;
			};

			partition@c0000 {
				label = "CDT";
				reg = <0xc0000 0x10000>;
				read-only;
			};

			partition@d0000 {
				label = "DDRPARAMS";
				reg = <0xd0000 0x10000>;
				read-only;
			};

			partition@e0000 {
				label = "APPSBLENV";
				reg = <0xe0000 0x10000>;
				read-only;
			};

			partition@f0000 {
				label = "APPSBL";
				reg = <0xf0000 0x80000>;
				read-only;
			};

			partition@170000 {
				label = "ART";
				reg = <0x170000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			partition@180000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x180000 0x1e80000>;
			};
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&crypto {
	status = "okay";
};

&gmac {
	status = "okay";
};

&mdio {
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&prng {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport1 {
	status = "okay";
};

&swport2 {
	status = "okay";
};

&swport3 {
	status = "okay";
};

&swport4 {
	status = "okay";
};

&swport5 {
	status = "okay";
};

&tlmm {
	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};
		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	serial_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pinmux {
			function = "blsp_spi0";
			pins = "gpio13", "gpio14", "gpio15";
			drive-strength = <12>;
			bias-disable;
		};

		pinmux_cs {
			function = "gpio";
			pins = "gpio12";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&usb2 {
	status = "okay";

	usb@6000000 {
		#address-cells = <1>;
		#size-cells = <0>;

		usb2_port1: port@1 {
			reg = <1>;
			#trigger-source-cells = <0>;
		};
	};
};

&usb2_hs_phy {
	status = "okay";
};

&usb3 {
	status = "okay";
};

&usb3_dwc {
	#address-cells = <1>;
	#size-cells = <0>;

	usb3_port1: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};

	usb3_port2: port@2 {
		reg = <2>;
		#trigger-source-cells = <0>;
	};
};

&usb3_hs_phy {
	status = "okay";
};

&usb3_ss_phy {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&wifi0 {
	status = "okay";
	nvmem-cells = <&precal_art_1000>;
	nvmem-cell-names = "pre-calibration";
	qcom,ath10k-calibration-variant = "YYeTs-LE1";
};

&wifi1 {
	status = "okay";
	nvmem-cells = <&precal_art_5000>;
	nvmem-cell-names = "pre-calibration";
	qcom,ath10k-calibration-variant = "YYeTs-LE1";
};
