# SPDX-License-Identifier: GPL-2.0-only
. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
actiontec,mi424wr-ac)
	# LAN ports connected to eth1 thru the KS8995 DSA switch
	ucidef_set_interface "eth" device "eth1" protocol "none"
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth0"
	;;
actiontec,mi424wr-d)
	# LAN ports connected to eth0 thru the KS8995 DSA switch
	ucidef_set_interface "eth" device "eth0" protocol "none"
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth1"
	;;
freecom,fsg-3|\
gateworks,gw2348|\
gateworks,gw2358)
	ucidef_set_interfaces_lan_wan "eth0" "eth1"
	;;
dlink,dsm-g600-a|\
iom,nas-100d|\
linksys,nslu2|\
netgear,wg302v1)
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
usr,usr8200)
	# LAN ports connected to eth1 thru the MV88E6060 DSA switch
	ucidef_set_interface "eth" device "eth1" protocol "none"
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth0"
	;;
*)
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
esac

board_config_flush

exit 0
