From d3eb58549842c60ed46f37da7f4da969e3d6ecd3 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Wed, 15 Jan 2025 14:45:00 +0000
Subject: [PATCH] net: phy: realtek: always clear NBase-T lpa

Clear NBase-T link partner advertisement before calling
rtlgen_read_status() to avoid phy_resolve_aneg_linkmode() wrongly
setting speed and duplex.

This fixes bogus 2.5G/5G/10G link partner advertisement and thus
speed and duplex being set by phy_resolve_aneg_linkmode() due to stale
NBase-T lpa.

Fixes: 68d5cd09e891 ("net: phy: realtek: change order of calls in C22 read_status()")
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Michal Swiatkowski <michal.swiatkowski@linux.intel.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/realtek.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/net/phy/realtek.c
+++ b/drivers/net/phy/realtek.c
@@ -960,15 +960,15 @@ static int rtl822x_read_status(struct ph
 {
 	int lpadv, ret;
 
+	mii_10gbt_stat_mod_linkmode_lpa_t(phydev->lp_advertising, 0);
+
 	ret = rtlgen_read_status(phydev);
 	if (ret < 0)
 		return ret;
 
 	if (phydev->autoneg == AUTONEG_DISABLE ||
-	    !phydev->autoneg_complete) {
-		mii_10gbt_stat_mod_linkmode_lpa_t(phydev->lp_advertising, 0);
+	    !phydev->autoneg_complete)
 		return 0;
-	}
 
 	lpadv = phy_read_paged(phydev, 0xa5d, 0x13);
 	if (lpadv < 0)
