#include "qcom-ipq8065-smb208.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Zyxel NBG6817";
	compatible = "zyxel,nbg6817", "qcom,ipq8065", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		mdio-gpio0 = &mdio0;
		sdcc1 = &sdcc1;

		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;
	};

	chosen {
		bootargs = "rootfstype=squashfs,ext4 rootwait noinitrd fstools_ignore_partname=1";
		append-rootblock = "root=/dev/mmcblk0p";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wifi {
			label = "wifi";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		internet {
			label = "white:internet";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_HIGH>;
		};

		power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		wifi2g {
			label = "amber:wifi2g";
			gpios = <&qcom_pinmux 33 GPIO_ACTIVE_HIGH>;
		};

		/* wifi2g amber from the manual is missing */

		wifi5g {
			label = "amber:wifi5g";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
		};

		/* wifi5g amber from the manual is missing */
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio53", "gpio54", "gpio65";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio9", "gpio26", "gpio33", "gpio64";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
		};
	};

	mdio0_pins: mdio0-state {
		/delete-property/ pins;
		/delete-property/ function;
		/delete-property/ drive-strength;
		/delete-property/ bias-disable;

		mux {
			pins = "gpio0", "gpio1";
			function = "mdio";
			drive-strength = <8>;
			bias-disable;
		};

		clk {
			pins = "gpio1";
			input-disable;
		};
	};

	rgmii2_pins: rgmii2-state {
		/delete-property/ pins;
		/delete-property/ function;
		/delete-property/ drive-strength;
		/delete-property/ bias-disable;

		mux {
			pins = "gpio27", "gpio28", "gpio29",
				"gpio30", "gpio31", "gpio32",
				"gpio51", "gpio52", "gpio59",
				"gpio60", "gpio61", "gpio62";
			function = "rgmii2";
			drive-strength = <8>;
			bias-disable;
		};

		tx {
			pins = "gpio27", "gpio28", "gpio29", "gpio30", "gpio31", "gpio32" ;
			input-disable;
		};
	};

	spi_pins: spi-state {
		/delete-property/ pins;
		/delete-property/ function;
		/delete-property/ drive-strength;
		/delete-property/ bias-disable;

		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			drive-strength = <10>;
			bias-disable;
		};

		cs {
			pins = "gpio20";
			drive-strength = <12>;
		};
	};

	usb0_pwr_en_pins: usb0_pwr_en_pins {
		mux {
			pins = "gpio16", "gpio17";
			function = "gpio";
			drive-strength = <12>;
		};

		pwr {
			pins = "gpio17";
			bias-pull-down;
			output-high;
		};

		ovc {
			pins = "gpio16";
			bias-pull-up;
		};
	};

	usb1_pwr_en_pins: usb1_pwr_en_pins {
		mux {
			pins = "gpio14", "gpio15";
			function = "gpio";
			drive-strength = <12>;
		};

		pwr {
			pins = "gpio14";
			bias-pull-down;
			output-high;
		};

		ovc {
			pins = "gpio15";
			bias-pull-up;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi4: spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_LOW>;

		m25p80@0 {
			compatible = "jedec,spi-nor";
			#address-cells = <1>;
			#size-cells = <1>;
			spi-max-frequency = <51200000>;
			reg = <0>;

			partitions {
				compatible = "qcom,smem-part";
			};
		};
	};
};

&hs_phy_0 {
	status = "okay";
};

&ss_phy_0 {
	status = "okay";
};

&usb3_0 {
	status = "okay";

	pinctrl-0 = <&usb0_pwr_en_pins>;
	pinctrl-names = "default";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";

	pinctrl-0 = <&usb1_pwr_en_pins>;
	pinctrl-names = "default";
};

&pcie0 {
	status = "okay";
	reset-gpios = <&qcom_pinmux 3 GPIO_ACTIVE_LOW>;
	pinctrl-0 = <&pcie0_pins>;
	pinctrl-names = "default";
};

&pcie1 {
	status = "okay";
	reset-gpios = <&qcom_pinmux 48 GPIO_ACTIVE_LOW>;
	pinctrl-0 = <&pcie1_pins>;
	pinctrl-names = "default";
	max-link-speed = <1>;
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	switch@10 {
		compatible = "qca,qca8337";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x10>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&gmac1>;
				phy-mode = "rgmii";
				tx-internal-delay-ps = <1000>;
				rx-internal-delay-ps = <1000>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			port@1 {
				reg = <1>;
				label = "lan1";
				phy-mode = "internal";
				phy-handle = <&phy_port1>;
			};

			port@2 {
				reg = <2>;
				label = "lan2";
				phy-mode = "internal";
				phy-handle = <&phy_port2>;
			};

			port@3 {
				reg = <3>;
				label = "lan3";
				phy-mode = "internal";
				phy-handle = <&phy_port3>;
			};

			port@4 {
				reg = <4>;
				label = "lan4";
				phy-mode = "internal";
				phy-handle = <&phy_port4>;
			};

			port@5 {
				reg = <5>;
				label = "wan";
				phy-mode = "internal";
				phy-handle = <&phy_port5>;
			};

			port@6 {
				reg = <6>;
				label = "cpu";
				ethernet = <&gmac2>;
				phy-mode = "sgmii";
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			phy_port1: phy@0 {
				reg = <0>;
			};

			phy_port2: phy@1 {
				reg = <1>;
			};

			phy_port3: phy@2 {
				reg = <2>;
			};

			phy_port4: phy@3 {
				reg = <3>;
			};

			phy_port5: phy@4 {
				reg = <4>;
			};
		};
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <1>;
	qcom,phy_mdio_addr = <4>;
	qcom,poll_required = <0>;
	qcom,rgmii_delay = <1>;
	qcom,phy_mii_type = <0>;
	qcom,emulation = <0>;
	qcom,irq = <255>;
	mdiobus = <&mdio0>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <2>;
	qcom,phy_mdio_addr = <0>;	/* none */
	qcom,poll_required = <0>;	/* no polling */
	qcom,rgmii_delay = <0>;
	qcom,phy_mii_type = <1>;
	qcom,emulation = <0>;
	qcom,irq = <258>;
	mdiobus = <&mdio0>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&sdcc1 {
	status = "okay";
};

&adm_dma {
	status = "okay";
};
