// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq8064-v2.0-smb208.dtsi"

#include <dt-bindings/input/input.h>

/ {
	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	reserved-memory {
		ramoops@42100000 {
			compatible = "ramoops";
			reg = <0x42100000 0x40000>;
			record-size = <0x4000>;
			console-size = <0x4000>;
			ftrace-size = <0x4000>;
			pmsg-size = <0x4000>;
		};
	};

	aliases {
		mdio-gpio0 = &mdio0;
		label-mac-device = &gmac2;
	};
};

&qcom_pinmux {
	spi_pins: spi_pins {
		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			bias-pull-down;
		};

		data {
			pins = "gpio18", "gpio19";
			drive-strength = <10>;
		};

		cs {
			pins = "gpio20";
			function = "gpio";
			drive-strength = <10>;
			bias-pull-up;
		};

		clk {
			pins = "gpio21";
			drive-strength = <12>;
		};
	};

	usb0_pwr_en_pin: usb0_pwr_en_pin {
		mux {
			pins = "gpio25";
			function = "gpio";
			drive-strength = <10>;
			bias-pull-up;
			output-high;
		};
	};

	usb1_pwr_en_pin: usb1_pwr_en_pin {
		mux {
			pins = "gpio23";
			function = "gpio";
			drive-strength = <10>;
			bias-pull-up;
			output-high;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_LOW>;

		flash@0 {
			compatible = "jedec,spi-nor";
			#address-cells = <1>;
			#size-cells = <1>;
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "SBL1";
					reg = <0x0 0x20000>;
					read-only;
				};

				partition@20000 {
					label = "MIBIB";
					reg = <0x20000 0x20000>;
					read-only;
				};

				partition@40000 {
					label = "SBL2";
					reg = <0x40000 0x20000>;
					read-only;
				};

				partition@60000 {
					label = "SBL3";
					reg = <0x60000 0x30000>;
					read-only;
				};

				partition@90000 {
					label = "DDRCONFIG";
					reg = <0x90000 0x10000>;
					read-only;
				};

				partition@a0000 {
					label = "SSD";
					reg = <0xa0000 0x10000>;
					read-only;
				};

				partition@b0000 {
					label = "TZ";
					reg = <0xb0000 0x30000>;
					read-only;
				};

				partition@e0000 {
					label = "RPM";
					reg = <0xe0000 0x20000>;
					read-only;
				};

				partition@100000 {
					label = "fs-uboot";
					reg = <0x100000 0x70000>;
					read-only;
				};

				partition@170000 {
					label = "uboot-env";
					reg = <0x170000 0x40000>;
					read-only;
				};

				partition@1b0000 {
					label = "radio";
					reg = <0x1b0000 0x40000>;
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						precal_radio_1000: precal@1000 {
							reg = <0x1000 0x2f20>;
						};

						precal_radio_5000: precal@5000 {
							reg = <0x5000 0x2f20>;
						};
					};
				};

				partition@1f0000 {
					label = "os-image";
					reg = <0x1f0000 0x400000>;
				};

				partition@5f0000 {
					label = "rootfs";
					reg = <0x5f0000 0x1900000>;
				};

				defaultmac: partition@1ef0000 {
					label = "default-mac";
					reg = <0x1ef0000 0x00200>;
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						macaddr_defaultmac_8: macaddr@8 {
							compatible = "mac-base";
							reg = <0x8 0x6>;
							#nvmem-cell-cells = <1>;
						};
					};
				};

				partition@1ef0200 {
					label = "pin";
					reg = <0x1ef0200 0x00200>;
					read-only;
				};

				partition@1ef0400 {
					label = "product-info";
					reg = <0x1ef0400 0x0fc00>;
					read-only;
				};

				partition@1f00000 {
					label = "partition-table";
					reg = <0x1f00000 0x10000>;
					read-only;
				};

				partition@1f10000 {
					label = "soft-version";
					reg = <0x1f10000 0x10000>;
					read-only;
				};

				partition@1f20000 {
					label = "support-list";
					reg = <0x1f20000 0x10000>;
					read-only;
				};

				partition@1f30000 {
					label = "profile";
					reg = <0x1f30000 0x10000>;
					read-only;
				};

				partition@1f40000 {
					label = "default-config";
					reg = <0x1f40000 0x10000>;
					read-only;
				};

				partition@1f50000 {
					label = "user-config";
					reg = <0x1f50000 0x40000>;
					read-only;
				};

				partition@1f90000 {
					label = "qos-db";
					reg = <0x1f90000 0x40000>;
					read-only;
				};

				partition@1fd0000 {
					label = "usb-config";
					reg = <0x1fd0000 0x10000>;
					read-only;
				};

				partition@1fe0000 {
					label = "log";
					reg = <0x1fe0000 0x20000>;
					read-only;
				};
			};
		};
	};
};

&hs_phy_0 {
	status = "okay";
};

&ss_phy_0 {
	status = "okay";
};

&usb3_0 {
	status = "okay";

	pinctrl-0 = <&usb0_pwr_en_pin>;
	pinctrl-names = "default";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";

	pinctrl-0 = <&usb1_pwr_en_pin>;
	pinctrl-names = "default";
};

&pcie0 {
	status = "okay";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "qcom,ath10k";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_defaultmac_8 (-1)>, <&precal_radio_1000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&pcie1 {
	status = "okay";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "qcom,ath10k";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_defaultmac_8 0>, <&precal_radio_5000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	switch@10 {
		compatible = "qca,qca8337";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x10>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&gmac1>;
				phy-mode = "rgmii";
				tx-internal-delay-ps = <1000>;
				rx-internal-delay-ps = <1000>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			port@1 {
				reg = <1>;
				label = "lan4";
				phy-mode = "internal";
				phy-handle = <&phy_port1>;
			};

			port@2 {
				reg = <2>;
				label = "lan3";
				phy-mode = "internal";
				phy-handle = <&phy_port2>;
			};

			port@3 {
				reg = <3>;
				label = "lan2";
				phy-mode = "internal";
				phy-handle = <&phy_port3>;
			};

			port@4 {
				reg = <4>;
				label = "lan1";
				phy-mode = "internal";
				phy-handle = <&phy_port4>;
			};

			port@5 {
				reg = <5>;
				label = "wan";
				phy-mode = "internal";
				phy-handle = <&phy_port5>;
			};

			port@6 {
				reg = <6>;
				label = "cpu";
				ethernet = <&gmac2>;
				phy-mode = "sgmii";
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			phy_port1: phy@0 {
				reg = <0>;
			};

			phy_port2: phy@1 {
				reg = <1>;
			};

			phy_port3: phy@2 {
				reg = <2>;
			};

			phy_port4: phy@3 {
				reg = <3>;
			};

			phy_port5: phy@4 {
				reg = <4>;
			};
		};
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	nvmem-cells = <&macaddr_defaultmac_8 1>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <2>;

	nvmem-cells = <&macaddr_defaultmac_8 0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&adm_dma {
	status = "okay";
};
