From 64ff63aeefb03139ae27454bd4208244579ae88e Mon Sep 17 00:00:00 2001
From: Aleksander Jan Bajkowski <olek2@wp.pl>
Date: Fri, 17 Jan 2025 23:24:21 +0100
Subject: [PATCH] net: phy: realtek: HWMON support for standalone versions of
 RTL8221B and RTL8251

HWMON support has been added for the RTL8221/8251 PHYs integrated together
with the MAC inside the RTL8125/8126 chips. This patch extends temperature
reading support for standalone variants of the mentioned PHYs.

I don't know whether the earlier revisions of the RTL8226 also have a
built-in temperature sensor, so they have been skipped for now.

Tested on RTL8221B-VB-CG.

Signed-off-by: Aleksander Jan Bajkowski <olek2@wp.pl>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/realtek/realtek_main.c | 5 +++++
 1 file changed, 5 insertions(+)

--- a/drivers/net/phy/realtek/realtek_main.c
+++ b/drivers/net/phy/realtek/realtek_main.c
@@ -1474,6 +1474,7 @@ static struct phy_driver realtek_drvs[]
 	}, {
 		.match_phy_device = rtl8221b_vb_cg_c22_match_phy_device,
 		.name           = "RTL8221B-VB-CG 2.5Gbps PHY (C22)",
+		.probe		= rtl822x_probe,
 		.get_features   = rtl822x_get_features,
 		.config_aneg    = rtl822x_config_aneg,
 		.config_init    = rtl822xb_config_init,
@@ -1486,6 +1487,7 @@ static struct phy_driver realtek_drvs[]
 	}, {
 		.match_phy_device = rtl8221b_vb_cg_c45_match_phy_device,
 		.name           = "RTL8221B-VB-CG 2.5Gbps PHY (C45)",
+		.probe		= rtl822x_probe,
 		.config_init    = rtl822xb_config_init,
 		.get_rate_matching = rtl822xb_get_rate_matching,
 		.get_features   = rtl822x_c45_get_features,
@@ -1496,6 +1498,7 @@ static struct phy_driver realtek_drvs[]
 	}, {
 		.match_phy_device = rtl8221b_vn_cg_c22_match_phy_device,
 		.name           = "RTL8221B-VM-CG 2.5Gbps PHY (C22)",
+		.probe		= rtl822x_probe,
 		.get_features   = rtl822x_get_features,
 		.config_aneg    = rtl822x_config_aneg,
 		.config_init    = rtl822xb_config_init,
@@ -1508,6 +1511,7 @@ static struct phy_driver realtek_drvs[]
 	}, {
 		.match_phy_device = rtl8221b_vn_cg_c45_match_phy_device,
 		.name           = "RTL8221B-VN-CG 2.5Gbps PHY (C45)",
+		.probe		= rtl822x_probe,
 		.config_init    = rtl822xb_config_init,
 		.get_rate_matching = rtl822xb_get_rate_matching,
 		.get_features   = rtl822x_c45_get_features,
@@ -1518,6 +1522,7 @@ static struct phy_driver realtek_drvs[]
 	}, {
 		.match_phy_device = rtl8251b_c45_match_phy_device,
 		.name           = "RTL8251B 5Gbps PHY",
+		.probe		= rtl822x_probe,
 		.get_features   = rtl822x_get_features,
 		.config_aneg    = rtl822x_config_aneg,
 		.read_status    = rtl822x_read_status,
