--- a/arch/arm/boot/dts/marvell/kirkwood-iconnect.dts
+++ b/arch/arm/boot/dts/marvell/kirkwood-iconnect.dts
@@ -8,6 +8,13 @@
 	model = "Iomega Iconnect";
 	compatible = "iom,iconnect-1.1", "iom,iconnect", "marvell,kirkwood-88f6281", "marvell,kirkwood";
 
+	aliases {
+		led-boot = &led_power_blue;
+		led-failsafe = &led_power_red;
+		led-running = &led_power_blue;
+		led-upgrade = &led_power_red;
+	};
+
 	memory {
 		device_type = "memory";
 		reg = <0x00000000 0x10000000>;
@@ -16,8 +23,6 @@
 	chosen {
 		bootargs = "console=ttyS0,115200n8 earlyprintk";
 		stdout-path = &uart0;
-		linux,initrd-start = <0x4500040>;
-		linux,initrd-end   = <0x4800000>;
 	};
 
 	ocp@f1000000 {
@@ -89,12 +94,12 @@
 			gpios = <&gpio1 9 GPIO_ACTIVE_HIGH>;
 			default-state = "on";
 		};
-		power-blue {
+		led_power_blue: power-blue {
 			label = "power:blue";
 			gpios = <&gpio1 10 GPIO_ACTIVE_HIGH>;
-			default-state = "keep";
+			default-state = "on";
 		};
-		power-red {
+		led_power_red: power-red {
 			label = "power:red";
 			gpios = <&gpio1 11 GPIO_ACTIVE_HIGH>;
 		};
@@ -146,28 +151,23 @@
 	status = "okay";
 
 	partition@0 {
-		label = "uboot";
-		reg = <0x0000000 0xc0000>;
+		label = "u-boot";
+		reg = <0x0000000 0xe0000>;
 	};
 
-	partition@a0000 {
-		label = "env";
-		reg = <0xa0000 0x20000>;
+	partition@e0000 {
+		label = "u-boot environment";
+		reg = <0xe0000 0x100000>;
 	};
 
 	partition@100000 {
-		label = "zImage";
-		reg = <0x100000 0x300000>;
-	};
-
-	partition@540000 {
-		label = "initrd";
-		reg = <0x540000 0x300000>;
+		label = "second stage u-boot";
+		reg = <0x100000 0x200000>;
 	};
 
-	partition@980000 {
-		label = "boot";
-		reg = <0x980000 0x1f400000>;
+	partition@200000 {
+		label = "ubi";
+		reg = <0x200000 0x1fe00000>;
 	};
 };
 
