From 3b2aef99221d395ce37efa426d7b50e7dcd621d6 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Mon, 1 Jul 2024 20:28:14 +0100
Subject: [PATCH] net: ethernet: mediatek: Allow gaps in MAC allocation

Some devices with MediaTek SoCs don't use the first but only the second
MAC in the chip. Especially with MT7981 which got a built-in 1GE PHY
connected to the second MAC this is quite common.
Make sure to reset and enable PSE also in those cases by skipping gaps
using 'continue' instead of aborting the loop using 'break'.

Fixes: dee4dd10c79a ("net: ethernet: mtk_eth_soc: ppe: add support for multiple PPEs")
Suggested-by: Elad Yifee <eladwf@gmail.com>
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Przemek Kitszel <przemyslaw.kitszel@intel.com>
Link: https://patch.msgid.link/379ae584cea112db60f4ada79c7e5ba4f3364a64.1719862038.git.daniel@makrotopia.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -3416,7 +3416,7 @@ static int mtk_open(struct net_device *d
 
 		for (i = 0; i < MTK_MAX_DEVS; i++) {
 			if (!eth->netdev[i])
-				break;
+				continue;
 
 			target_mac = netdev_priv(eth->netdev[i]);
 			if (!soc->offload_version) {
