--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -51,6 +51,17 @@ config HIVEAP_330
       This board is a Concurrent Dual-Band wireless access point with a
       Freescale P1020 SoC.
 
+config PANDA
+	bool "OCEDO PANDA"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	help
+	  This option enables support for the OCEDO PANDA board.
+
+	  This board is a Concurrent Dual-Band wireless access point with a
+	  Freescale P1020 SoC.
+
 config MPC8540_ADS
 	bool "Freescale MPC8540 ADS"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -22,6 +22,7 @@ obj-$(CONFIG_P1010_RDB)   += p1010rdb.o
 obj-$(CONFIG_P1022_DS)    += p1022_ds.o
 obj-$(CONFIG_P1022_RDK)   += p1022_rdk.o
 obj-$(CONFIG_P1023_RDB)   += p1023_rdb.o
+obj-$(CONFIG_PANDA)       += panda.o
 obj-$(CONFIG_PPC_P2020)   += p2020.o $(obj8259-y)
 obj-$(CONFIG_TWR_P102x)   += twr_p102x.o
 obj-$(CONFIG_CORENET_GENERIC)   += corenet_generic.o
