#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "hiwifi,hc5962", "mediatek,mt7621-soc";
	model = "HiWiFi HC5962";

	aliases {
		label-mac-device = &gmac0;
		led-boot = &led_status_red;
		led-failsafe = &led_status_red;
		led-running = &led_status_white;
		led-upgrade = &led_status_white;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	leds {
		compatible = "gpio-leds";

		led_status_white: led-0 {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		led_status_red: led-1 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			panic-indicator;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};
	};

	ubi-concat {
		compatible = "mtd-concat";
		devices = <&ubiconcat0 &ubiconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x0 0x79c0000>;
			};
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "debug";
			reg = <0x80000 0x80000>;
			read-only;
		};

		partition@100000 {
			label = "factory";
			reg = <0x100000 0x40000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0x400>;
				};

				eeprom_factory_8000: eeprom@8000 {
					reg = <0x8000 0x200>;
				};
			};
		};

		partition@140000 {
			label = "kernel";
			reg = <0x140000 0x400000>;
		};

		ubiconcat0: partition@540000 {
			label = "ubiconcat0";
			reg = <0x540000 0x1c80000>;
		};

		partition@21c0000 {
			label = "bdinfo";
			reg = <0x21c0000 0x80000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_bdinfo_18a: macaddr@18a {
					compatible = "mac-base";
					reg = <0x18a 0x11>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		ubiconcat1: partition@2240000 {
			label = "ubiconcat1";
			reg = <0x2240000 0x5d40000>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>, <&macaddr_bdinfo_18a 0>;
		nvmem-cell-names = "eeprom", "mac-address";
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_8000>, <&macaddr_bdinfo_18a 0>;
		nvmem-cell-names = "eeprom", "mac-address";
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_bdinfo_18a 0>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_bdinfo_18a 1>;
	nvmem-cell-names = "mac-address";
};

&ethphy4 {
	/delete-property/ interrupts;
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan1";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan3";
		};
	};
};

&state_default {
	gpio {
		groups = "uart3", "jtag";
		function = "gpio";
	};
};
