
. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
meraki,mr24|\
wd,mybooklive|\
wd,mybooklive-duo)
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
netgear,wndap620)
	ucidef_add_switch "switch0" "2:lan" "5@eth0"
	;;
netgear,wndap660)
	ucidef_add_switch "switch0" "1:lan" "2:lan" "5@eth0"
	;;
meraki,mx60|\
netgear,wndr4700)
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "wan"
	;;

*)
	ucidef_set_interfaces_lan_wan "eth0" "eth1"
	;;
esac

board_config_flush

exit 0
