From 38093ebbf25eb60a1aa863f46118a68a0300c56e Mon Sep 17 00:00:00 2001
From: Kuldeep Singh <kuldeep.singh@nxp.com>
Date: Fri, 3 Jan 2020 14:49:07 +0530
Subject: [PATCH] arm64: dts: ls1046a-rdb: Update qspi spi-rx-bus-width to 1

Update rx width from quad mode to single mode as a workaround.

[Leo: Local workaround ]

Signed-off-by: Kuldeep Singh <kuldeep.singh@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb.dts
@@ -104,7 +104,7 @@
 		#address-cells = <1>;
 		#size-cells = <1>;
 		spi-max-frequency = <50000000>;
-		spi-rx-bus-width = <4>;
+		spi-rx-bus-width = <1>;
 		spi-tx-bus-width = <1>;
 		reg = <0>;
 	};
@@ -114,7 +114,7 @@
 		#address-cells = <1>;
 		#size-cells = <1>;
 		spi-max-frequency = <50000000>;
-		spi-rx-bus-width = <4>;
+		spi-rx-bus-width = <1>;
 		spi-tx-bus-width = <1>;
 		reg = <1>;
 	};
