#include "mt7620a_hiwifi_hc5x61.dtsi"

/ {
	compatible = "hiwifi,hc5861", "ralink,mt7620a-soc";
	model = "HiWiFi HC5861";

	aliases {
		label-mac-device = &ethernet;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	leds {
		compatible = "gpio-leds";

		led_status: led-0 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		led-1 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN_2GHZ;
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led-2 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
		};

		led-3 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN_5GHZ;
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-4 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_USB;
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "usbport";
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
		};
	};

	gpio_export {
		compatible = "gpio-export";

		usbpower {
			gpio-export,name = "usbpower";
			gpio-export,output = <0>;
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&ethernet {
	pinctrl-names = "default";
	pinctrl-0 = <&mdio_pins>, <&rgmii1_pins>;

	mediatek,portmap = "llllw";

	port@5 {
		status = "okay";
		phy-handle = <&phy5>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy5: ethernet-phy@5 {
			reg = <5>;
			phy-mode = "rgmii";
		};
	};
};

&gsw {
	mediatek,ephy-base = /bits/ 8 <12>;
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_8000>, <&macaddr_bdinfo_18a 0>;
		nvmem-cell-names = "eeprom", "mac-address";
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&reg_vmmc {
	gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
};

&wmac {
	pinctrl-names = "default", "pa_gpio";
	pinctrl-0 = <&pa_pins>;
	pinctrl-1 = <&pa_gpio_pins>;
};
