From fecb65813ddf52abf310bc2227a0ac869dc897d1 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Wed, 29 Jan 2025 14:47:41 +0100
Subject: [PATCH 1/3] airoha: ethernet: drop xsi-mac reset

In preparation for support for Ethernet and PON PCS, drop the xsi-mac
reset from airoha_eth. This reset is related to the Ethernet PCS and
should be handled in the dedicated driver.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/net/ethernet/airoha/airoha_eth.c | 9 ++++-----
 drivers/net/ethernet/airoha/airoha_eth.h | 2 +-
 2 files changed, 5 insertions(+), 6 deletions(-)

--- a/drivers/net/ethernet/airoha/airoha_eth.c
+++ b/drivers/net/ethernet/airoha/airoha_eth.c
@@ -3100,7 +3100,6 @@ static void airoha_remove(struct platfor
 }
 
 static const char * const en7581_xsi_rsts_names[] = {
-	"xsi-mac",
 	"hsi0-mac",
 	"hsi1-mac",
 	"hsi-mac",
@@ -3132,7 +3131,6 @@ static int airoha_en7581_get_src_port_id
 }
 
 static const char * const an7583_xsi_rsts_names[] = {
-	"xsi-mac",
 	"hsi0-mac",
 	"hsi1-mac",
 	"xfp-mac",
