// SPDX-License-Identifier: GPL-2.0-or-later

#include "qcom-ipq8065-smb208.dtsi"
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Arris TR4400 v2";
	compatible = "arris,tr4400-v2", "qcom,ipq8065", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		led-boot = &led_status_blue;
		led-failsafe = &led_status_red;
		led-running = &led_status_blue;
		led-upgrade = &led_status_red;
	};

	chosen {
		bootargs = "rootfstype=squashfs noinitrd";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		led_status_red: status_red {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_RED>;
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		led_status_blue: status_blue {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio6", "gpio54";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio7", "gpio8";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
		};
	};

	rgmii2_pins: rgmii2-pins {
		tx {
			pins = "gpio27", "gpio28", "gpio29", "gpio30", "gpio31", "gpio32";
			input-disable;
		};
	};

	spi_pins: spi_pins {
		cs {
			pins = "gpio20";
			drive-strength = <12>;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_LOW>;

		flash@0 {
			compatible = "everspin,mr25h256";
			spi-max-frequency = <40000000>;
			reg = <0>;
		};
	};
};

&nand {
	status = "okay";

	nand@0 {
		reg = <0>;
		compatible = "qcom,nandcs";

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;
		nand-ecc-step-size = <512>;

		qcom,boot-partitions = <0x0 0x1180000 0x5340000 0x10c0000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "0:SBL1";
				reg = <0x0000000 0x0040000>;
				read-only;
			};
			partition@40000 {
				label = "0:MIBIB";
				reg = <0x0040000 0x0140000>;
				read-only;
			};
			partition@180000 {
				label = "0:SBL2";
				reg = <0x0180000 0x0140000>;
				read-only;
			};
			partition@2c0000 {
				label = "0:SBL3";
				reg = <0x02c0000 0x0280000>;
				read-only;
			};
			partition@540000 {
				label = "0:DDRCONFIG";
				reg = <0x0540000 0x0120000>;
				read-only;
			};
			partition@660000 {
				label = "0:SSD";
				reg = <0x0660000 0x0120000>;
				read-only;
			};
			partition@780000 {
				label = "0:TZ";
				reg = <0x0780000 0x0280000>;
				read-only;
			};
			partition@a00000 {
				label = "0:RPM";
				reg = <0x0a00000 0x0280000>;
				read-only;
			};
			partition@c80000 {
				label = "0:APPSBL";
				reg = <0x0c80000 0x0500000>;
				read-only;
			};
			partition@1180000 {
				label = "0:APPSBLENV";
				reg = <0x1180000 0x0080000>;
			};
			partition@1200000 {
				label = "0:ART";
				reg = <0x1200000 0x0140000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_ART_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};
					precal_ART_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
			partition@1340000 {
				label = "extra";
				reg = <0x1340000 0x4000000>;
			};
			partition@5340000 {
				label = "0:BOOTCONFIG";
				reg = <0x5340000 0x0060000>;
				read-only;
			};
			partition@53a0000 {
				label = "0:SBL2_1";
				reg = <0x53a0000 0x0140000>;
				read-only;
			};
			partition@54e0000 {
				label = "0:SBL3_1";
				reg = <0x54e0000 0x0280000>;
				read-only;
			};
			partition@5760000 {
				label = "0:DDRCONFIG_1";
				reg = <0x5760000 0x0120000>;
				read-only;
			};
			partition@5880000 {
				label = "0:SSD_1";
				reg = <0x5880000 0x0120000>;
				read-only;
			};
			partition@59a0000 {
				label = "0:TZ_1";
				reg = <0x59a0000 0x0280000>;
				read-only;
			};
			partition@5c20000 {
				label = "0:RPM_1";
				reg = <0x5c20000 0x0280000>;
				read-only;
			};
			partition@5ea0000 {
				label = "0:BOOTCONFIG1";
				reg = <0x5ea0000 0x0060000>;
				read-only;
			};
			partition@5f00000 {
				label = "0:APPSBL_1";
				reg = <0x5f00000 0x0500000>;
				read-only;
			};
			partition@6400000 {
				label = "fw_env";
				reg = <0x6400000 0x0100000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_fw_env_0: macaddr@0 {
						reg = <0x00 0x6>;
					};
					macaddr_fw_env_6: macaddr@6 {
						reg = <0x06 0x6>;
					};
					macaddr_fw_env_c: macaddr@c {
						reg = <0x0c 0x6>;
					};
					macaddr_fw_env_12: macaddr@12 {
						reg = <0x12 0x6>;
					};
					macaddr_fw_env_18: macaddr@18 {
						reg = <0x18 0x6>;
					};
				};
			};
			partition@6500000 {
				label = "ubi";
				reg = <0x6500000 0x9b00000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	switch@10 {
		compatible = "qca,qca8337";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x10>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&gmac0>;
				phy-mode = "rgmii";
				tx-internal-delay-ps = <1000>;
				rx-internal-delay-ps = <1000>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			port@1 {
				reg = <1>;
				label = "lan1";
				phy-mode = "internal";
				phy-handle = <&phy_port1>;
			};

			port@2 {
				reg = <2>;
				label = "lan2";
				phy-mode = "internal";
				phy-handle = <&phy_port2>;
			};

			port@3 {
				reg = <3>;
				label = "lan3";
				phy-mode = "internal";
				phy-handle = <&phy_port3>;
			};

			port@4 {
				reg = <4>;
				label = "lan4";
				phy-mode = "internal";
				phy-handle = <&phy_port4>;
			};

			port@6 {
				reg = <6>;
				label = "cpu";
				ethernet = <&gmac1>;
				phy-mode = "sgmii";
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			phy_port1: phy@0 {
				reg = <0>;
			};

			phy_port2: phy@1 {
				reg = <1>;
			};

			phy_port3: phy@2 {
				reg = <2>;
			};

			phy_port4: phy@3 {
				reg = <3>;
			};
		};
	};

	phy7: ethernet-phy@7 {
		reg = <7>;
	};
};

&gmac0 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <0>;

	nvmem-cells = <&macaddr_fw_env_18>;
	nvmem-cell-names = "mac-address";

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <1>;

	nvmem-cells = <&macaddr_fw_env_0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac3 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <3>;
	phy-handle = <&phy7>;

	nvmem-cells = <&macaddr_fw_env_6>;
	nvmem-cell-names = "mac-address";
};

&adm_dma {
	status = "okay";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";
	reset-gpios = <&qcom_pinmux 3 GPIO_ACTIVE_HIGH>;
	pinctrl-0 = <&pcie0_pins>;
	pinctrl-names = "default";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi0: wifi@1,0 {
			compatible = "qcom,ath10k";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&precal_ART_1000>, <&macaddr_fw_env_12>;
			nvmem-cell-names = "pre-calibration", "mac-address";
		};
	};
};

&pcie1 {
	status = "okay";
	reset-gpios = <&qcom_pinmux 48 GPIO_ACTIVE_HIGH>;
	pinctrl-0 = <&pcie1_pins>;
	pinctrl-names = "default";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi1: wifi@1,0 {
			compatible = "qcom,ath10k";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&precal_ART_5000>, <&macaddr_fw_env_c>;
			nvmem-cell-names = "pre-calibration", "mac-address";
		};
	};
};
