#include "danube.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "arcadyan,arv7518pw", "lantiq,xway", "lantiq,danube";
	model = "Astoria Networks ARV7518PW";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl;
		led-internet = &online_green;
		led-usb = &led_usb;
		led-wifi = &wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		rfkill {
			label = "rfkill";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		power_green: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		dsl: dsl {
			label = "green:dsl";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		online_green: online {
			label = "green:internet";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		power_red: power2 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};
		online2 {
			label = "red:internet";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		led_usb: usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
		voice {
			label = "green:voip";
			gpios = <&gpiomm 0 GPIO_ACTIVE_LOW>;
		};
		fxs1 {
			label = "green:phone1";
			gpios = <&gpiomm 1 GPIO_ACTIVE_LOW>;
		};
		fxs2 {
			label = "green:phone2";
			gpios = <&gpiomm 2 GPIO_ACTIVE_LOW>;
		};
		unlabeled {
			label = "amber:unlabeled";
			gpios = <&gpiomm 3 GPIO_ACTIVE_LOW>;
		};
		wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpiomm 4 GPIO_ACTIVE_LOW>;
		};
		wps2 {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpiomm 5 GPIO_ACTIVE_LOW>;
		};
		wps3 {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpiomm 6 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		ebu {
			lantiq,groups = "ebu cs1";
			lantiq,function = "ebu";
		};
		pci_rst {
			lantiq,pins = "io21";
			lantiq,pull = <2>;
			lantiq,output = <1>;
		};
		leds {
			lantiq,pins = "io2", "io4", "io5", "io6", "io7", "io8", "io19";
			lantiq,output = <1>;
		};
		keys {
			lantiq,pins = "io28", "io30";
			lantiq,output = <0>;
			lantiq,pull = <2>;
			lantiq,open-drain = <1>;
		};
	};
};

/*
#define SWITCH_RESET          13
*/
&gsw {
	phy-mode = "mii";
	nvmem-cells = <&macaddr_boardconfig_16 0>;
	nvmem-cell-names = "mac-address";
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x2000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x10000>;
				read-only;
			};

			partition@10000 {
				label = "u-boot-env";
				reg = <0x10000 0x10000>;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0x7d0000>;
			};

			boardconfig: partition@7f0000 {
				label = "boardconfig";
				reg = <0x7f0000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_boardconfig_16: macaddr@16 {
						compatible = "mac-base";
						reg = <0x16 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};
		};
	};

	gpiomm: gpio@1 {
		compatible = "lantiq,gpio-mm";
		reg = <1 0x0 0x10 >;
		#address-cells = <1>;
		#size-cells = <1>;
		#gpio-cells = <2>;
		gpio-controller;
		lantiq,shadow = <0x0>;
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>;
	pinctrl-names = "default";

	reset-gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
	lantiq,external-clock;
	req-mask = <0xf>;

	wifi@168c,0029 {
		compatible = "pci168c,0029";
		reg = <0x7000 0 0 0 0>;
		qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:00:0e.0.bin */
		nvmem-cells = <&macaddr_boardconfig_16 1>;
		nvmem-cell-names = "mac-address";
	};
};

&usb_phy {
	status = "okay";
};

&usb {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&vmmc {
	status = "okay";
};
